| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5454: Machine instructions VSCATTERPF0DPS VSCATTERPF0HINTDPS VSCATTERPF0QPS VSCATTERPF0DPD VSCATTERPF0HINTDPD VSCATTERPF0QPD

Tested procedures
  IizVSCATTERPF0DPS IizVSCATTERPF0HINTDPS IizVSCATTERPF0QPS IizVSCATTERPF0DPD IizVSCATTERPF0HINTDPD IizVSCATTERPF0QPD

Source & expected listing t5454.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5454 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F27D4BC76C0D10<2 | VSCATTERPF0QPS [ZMM1+RBP+40h],MASK=K3 |00000008:62F2FD4BC76C0D08<3 | VSCATTERPF0QPD [ZMM1+RBP+40h],MASK=K3 |00000010:62F2FD4BC66C0D08<3 | VSCATTERPF0DPD [YMM1+RBP+40h],MASK=K3 |00000018:62F27D4BC66C0D10<2 | VSCATTERPF0DPS [ZMM1+RBP+40h],MASK=K3 |00000020:62F2790BC66C0D10<2 | VSCATTERPF0DPS [ZMM1+RBP+40h],MASK=K3,PREFIX=MVEX |00000028:62F2790BC6640D10<2 | VSCATTERPF0HINTDPS [ZMM1+RBP+40h],MASK=K3 |00000030:62F2F90BC6640D08<3 | VSCATTERPF0HINTDPD [ZMM1+RBP+40h],MASK=K3 | |ENDPROGRAM t5454`

Expected messages t5454.out
  `I0180 Assembling source file "t5454.htm". I0270 Assembling source "t5454". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5454". "t5454.htm"{64} I0510 Assembling program pass 1. "t5454.htm"{64} I0530 Assembling program pass 2 - final. "t5454.htm"{64} I0660 16bit TINY BIN file "t5454.bin" created, size=56. "t5454.htm"{73} I0650 Program "t5454" assembled in 2 passes with errorlevel 0. "t5454.htm"{73} I0750 Source "t5454" (91 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5454.htm.lst" created, size=818. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲