| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3112: Machine instructions ADC ADCB ADCW ADCD in 32bit mode

Tested procedures
  IigADC IigADCB IigADCW IigADCD

Source & expected listing t3112.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3112 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:1402 | ADC AL,2 |00000002:80D002 | ADC AL,2,CODE=LONG |00000005:66150200 | ADC AX,2 |00000009:6683D002 | ADC AX,2,CODE=LONG |0000000D:83D002 | ADC EAX,2 |00000010:1502000000 | ADC EAX,2,CODE=SHORT |00000015:80D102 | ADC CL,2 |00000018:8015[AE000000]02 | ADC [MemByte],2 |0000001F:6683D102 | ADC CX,2 |00000023:6681D10200 | ADC CX,2,IMM=WORD |00000028:668315[AC000000]02 | ADC [MemWord],2 |00000030:668115[AC000000]0200 | ADC [MemWord],2,IMM=WORD |00000039:8115[AC000000]02000000 | ADCD [MemWord],2,IMM=DWORD |00000043:83D102 | ADC ECX,2 |00000046:81D102000000 | ADC ECX,2,IMM=DWORD |0000004C:8315[A8000000]02 | ADC [MemDword],2 |00000053:668315[A8000000]02 | ADCW [MemDword],2 |0000005B:8115[A8000000]02000000 | ADC [MemDword],2,IMM=DWORD |00000065:801702 | ADCB [EDI],2 |00000068:66831702 | ADCW [EDI],2 |0000006C:831702 | ADCD [EDI],2 |0000006F:10D1 | ADC CL,DL |00000071:12CA | ADC CL,DL,CODE=LONG |00000073:10F5 | ADC CH,DH |00000075:12EE | ADC CH,DH,CODE=LONG |00000077:6611D1 | ADC CX,DX |0000007A:6613CA | ADC CX,DX,CODE=LONG |0000007D:11D1 | ADC ECX,EDX |0000007F:13CA | ADC ECX,EDX,CODE=LONG |00000081:120D[AE000000] | ADC CL,[MemByte] |00000087:66130D[AC000000] | ADC CX,[MemWord] |0000008E:130D[A8000000] | ADC ECX,[MemDword] |00000094:1015[AE000000] | ADC [MemByte],DL |0000009A:661115[AC000000] | ADC [MemWord],DX |000000A1:1115[A8000000] | ADC [MemDword],EDX |000000A7:90 | ALIGN QWORD |000000A8:00000000 |MemDword D D |000000AC:0000 |MemWord D W |000000AE:00 |MemByte D B | |ENDPROGRAM t3112`

Expected messages t3112.out
  `I0180 Assembling source file "t3112.htm". I0270 Assembling source "t3112". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3112". "t3112.htm"{58} I0510 Assembling program pass 1. "t3112.htm"{58} I0510 Assembling program pass 2. "t3112.htm"{58} I0510 Assembling program pass 3. "t3112.htm"{58} I0530 Assembling program pass 4 - final. "t3112.htm"{58} I0660 16bit TINY BIN file "t3112.bin" created, size=175. "t3112.htm"{99} I0650 Program "t3112" assembled in 4 passes with errorlevel 0. "t3112.htm"{99} I0750 Source "t3112" (119 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3112.htm.lst" created, size=2413. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲