| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3103: Machine instructions SBB SBBB SBBW SBBD SBBQ in 16bit mode

Tested procedures
  IigSBB IigSBBB IigSBBW IigSBBD IigSBBQ

Source & expected listing t3103.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3103 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:1C02 | SBB AL,2 |0002:80D802 | SBB AL,2,CODE=LONG |0005:1D0200 | SBB AX,2 |0008:83D802 | SBB AX,2,CODE=LONG |000B:6683D802 | SBB EAX,2 |000F:661D02000000 | SBB EAX,2,CODE=SHORT |0015:80D902 | SBB CL,2 |0018:801E[8600]02 | SBB [MemByte],2 |001D:83D902 | SBB CX,2 |0020:81D90200 | SBB CX,2,IMM=WORD |0024:831E[8400]02 | SBB [MemWord],2 |0029:811E[8400]0200 | SBB [MemWord],2,IMM=WORD |002F:6683D902 | SBB ECX,2 |0033:6681D902000000 | SBB ECX,2,IMM=DWORD |003A:66831E[8000]02 | SBB [MemDword],2 |0040:66811E[8000]02000000 | SBB [MemDword],2,IMM=DWORD |0049:801D02 | SBBB [DI],2 |004C:831D02 | SBBW [DI],2 |004F:66831D02 | SBBD [DI],2 |0053:18D1 | SBB CL,DL |0055:1ACA | SBB CL,DL,CODE=LONG |0057:18F5 | SBB CH,DH |0059:1AEE | SBB CH,DH,CODE=LONG |005B:19D1 | SBB CX,DX |005D:1BCA | SBB CX,DX,CODE=LONG |005F:6619D1 | SBB ECX,EDX |0062:661BCA | SBB ECX,EDX,CODE=LONG |0065:1A0E[8600] | SBB CL,[MemByte] |0069:1B0E[8400] | SBB CX,[MemWord] |006D:661B0E[8000] | SBB ECX,[MemDword] |0072:1816[8600] | SBB [MemByte],DL |0076:1916[8400] | SBB [MemWord],DX |007A:661916[8000] | SBB [MemDword],EDX |007F:90 | ALIGN QWORD |0080:00000000 |MemDword D D |0084:0000 |MemWord D W |0086:00 |MemByte D B | |ENDPROGRAM t3103`

Expected messages t3103.out
  `I0180 Assembling source file "t3103.htm". I0270 Assembling source "t3103". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3103". "t3103.htm"{61} I0510 Assembling program pass 1. "t3103.htm"{61} I0510 Assembling program pass 2. "t3103.htm"{61} I0510 Assembling program pass 3. "t3103.htm"{61} I0530 Assembling program pass 4 - final. "t3103.htm"{61} I0660 16bit TINY BIN file "t3103.bin" created, size=135. "t3103.htm"{100} I0650 Program "t3103" assembled in 4 passes with errorlevel 0. "t3103.htm"{100} I0750 Source "t3103" (120 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3103.htm.lst" created, size=2289. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲