| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5618: Machine instructions VPADDUSB VPADDUSW VPSUBUSB VPSUBUSW

Tested procedures
  IizVPADDUSB IizVPADDUSW IizVPSUBUSB IizVPSUBUSW

Source & expected listing t5618.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON | |t5618 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5E9DCCB | VPADDUSB XMM1,XMM2,XMM3 |00000004:C5EDDCCB | VPADDUSB YMM1,YMM2,YMM3 |00000008:C4E169DCCB | VPADDUSB XMM1,XMM2,XMM3,PREFIX=VEX3 |0000000D:C4E16DDCCB | VPADDUSB YMM1,YMM2,YMM3,PREFIX=VEX3 |00000012:62F16D0CDCCB | VPADDUSB XMM1,XMM2,XMM3,MASK=K4 |00000018:62F16DACDCCB | VPADDUSB YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000001E:62F16DCCDCCB | VPADDUSB ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000024:C5E9DC4D40 | VPADDUSB XMM1,XMM2,[RBP+40h] |00000029:C5EDDC4D40 | VPADDUSB YMM1,YMM2,[RBP+40h] |0000002E:C4E169DC4D40 | VPADDUSB XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000034:C4E16DDC4D40 | VPADDUSB YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |0000003A:62F16D48DC4D01<6 | VPADDUSB ZMM1,ZMM2,[RBP+40h] |00000041:62F16D0CDC4D04<4 | VPADDUSB XMM1,XMM2,[RBP+40h],MASK=K4 |00000048:62F16DACDC4D02<5 | VPADDUSB YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000004F:62F16DCCDC4D01<6 | VPADDUSB ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000056:C5E9DDCB | VPADDUSW XMM1,XMM2,XMM3 |0000005A:C5EDDDCB | VPADDUSW YMM1,YMM2,YMM3 |0000005E:C4E169DDCB | VPADDUSW XMM1,XMM2,XMM3,PREFIX=VEX3 |00000063:C4E16DDDCB | VPADDUSW YMM1,YMM2,YMM3,PREFIX=VEX3 |00000068:62F16D0CDDCB | VPADDUSW XMM1,XMM2,XMM3,MASK=K4 |0000006E:62F16DACDDCB | VPADDUSW YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000074:62F16DCCDDCB | VPADDUSW ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |0000007A:C5E9DD4D40 | VPADDUSW XMM1,XMM2,[RBP+40h] |0000007F:C5EDDD4D40 | VPADDUSW YMM1,YMM2,[RBP+40h] |00000084:C4E169DD4D40 | VPADDUSW XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |0000008A:C4E16DDD4D40 | VPADDUSW YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |00000090:62F16D48DD4D01<6 | VPADDUSW ZMM1,ZMM2,[RBP+40h] |00000097:62F16D0CDD4D04<4 | VPADDUSW XMM1,XMM2,[RBP+40h],MASK=K4 |0000009E:62F16DACDD4D02<5 | VPADDUSW YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000A5:62F16DCCDD4D01<6 | VPADDUSW ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000AC:C5E9D8CB | VPSUBUSB XMM1,XMM2,XMM3 |000000B0:C5EDD8CB | VPSUBUSB YMM1,YMM2,YMM3 |000000B4:C4E169D8CB | VPSUBUSB XMM1,XMM2,XMM3,PREFIX=VEX3 |000000B9:C4E16DD8CB | VPSUBUSB YMM1,YMM2,YMM3,PREFIX=VEX3 |000000BE:62F16D0CD8CB | VPSUBUSB XMM1,XMM2,XMM3,MASK=K4 |000000C4:62F16DACD8CB | VPSUBUSB YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |000000CA:62F16DCCD8CB | VPSUBUSB ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |000000D0:C5E9D84D40 | VPSUBUSB XMM1,XMM2,[RBP+40h] |000000D5:C5EDD84D40 | VPSUBUSB YMM1,YMM2,[RBP+40h] |000000DA:C4E169D84D40 | VPSUBUSB XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |000000E0:C4E16DD84D40 | VPSUBUSB YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |000000E6:62F16D48D84D01<6 | VPSUBUSB ZMM1,ZMM2,[RBP+40h] |000000ED:62F16D0CD84D04<4 | VPSUBUSB XMM1,XMM2,[RBP+40h],MASK=K4 |000000F4:62F16DACD84D02<5 | VPSUBUSB YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000FB:62F16DCCD84D01<6 | VPSUBUSB ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000102:C5E9D9CB | VPSUBUSW XMM1,XMM2,XMM3 |00000106:C5EDD9CB | VPSUBUSW YMM1,YMM2,YMM3 |0000010A:C4E169D9CB | VPSUBUSW XMM1,XMM2,XMM3,PREFIX=VEX3 |0000010F:C4E16DD9CB | VPSUBUSW YMM1,YMM2,YMM3,PREFIX=VEX3 |00000114:62F16D0CD9CB | VPSUBUSW XMM1,XMM2,XMM3,MASK=K4 |0000011A:62F16DACD9CB | VPSUBUSW YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000120:62F16DCCD9CB | VPSUBUSW ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000126:C5E9D94D40 | VPSUBUSW XMM1,XMM2,[RBP+40h] |0000012B:C5EDD94D40 | VPSUBUSW YMM1,YMM2,[RBP+40h] |00000130:C4E169D94D40 | VPSUBUSW XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000136:C4E16DD94D40 | VPSUBUSW YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |0000013C:62F16D48D94D01<6 | VPSUBUSW ZMM1,ZMM2,[RBP+40h] |00000143:62F16D0CD94D04<4 | VPSUBUSW XMM1,XMM2,[RBP+40h],MASK=K4 |0000014A:62F16DACD94D02<5 | VPSUBUSW YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000151:62F16DCCD94D01<6 | VPSUBUSW ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON | |ENDPROGRAM t5618`

Expected messages t5618.out
  `I0180 Assembling source file "t5618.htm". I0270 Assembling source "t5618". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5618". "t5618.htm"{58} I0510 Assembling program pass 1. "t5618.htm"{58} I0530 Assembling program pass 2 - final. "t5618.htm"{58} I0660 16bit TINY BIN file "t5618.bin" created, size=344. "t5618.htm"{120} I0650 Program "t5618" assembled in 2 passes with errorlevel 0. "t5618.htm"{120} I0750 Source "t5618" (138 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5618.htm.lst" created, size=4380. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲