| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t7121: OutFile sublist

Description
  72 bytes of binary data are compiled in memory. The output file is suboperated, its first two lines are omitted.
Tested procedures
  PfSuboperate

Source & expected listing t7121.htm.lst
  `| | EUROASM DEBUG=OFF,PROFILE=OFF,AUTOSEGMENT=ON,LIST=ON, \ | | DUMP=ON,DUMPWIDTH=40,DUMPALL=ON | |t7121 PROGRAM FORMAT=BIN,MODEL=TINY,WIDTH=16, \ | | LISTMAP=OFF,LISTGLOBALS=OFF,OUTFILE="t7121.bin"{3..%&} |[DATA] |[DATA] |0000:41314132413341344135413641370D0A | DB "A1A2A3A4A5A6A7",13,10 |0010:42314232423342344235423642370D0A | DB "B1B2B3B4B5B6B7",13,10 |0020:43314332433343344335433643370D0A | DB "C1C2C3C4C5C6C7",13,10 |0030:44314432443344344435443644370D0A | DB "D1D2D3D4D5D6D7",13,10 |0040:4531453245334534 | DB "E1E2E3E4" | | ENDPROGRAM t7121`

Expected messages t7121.out
  `I0180 Assembling source file "t7121.htm". I0270 Assembling source "t7121". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t7121". "t7121.htm"{53} I0510 Assembling program pass 1. "t7121.htm"{53} I0530 Assembling program pass 2 - final. "t7121.htm"{53} I0660 16bit TINY BIN file "t7121.bin" created, size=40. "t7121.htm"{61} I0650 Program "t7121" assembled in 2 passes with errorlevel 0. "t7121.htm"{61} I0750 Source "t7121" (86 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t7121.htm.lst" created, size=859. I0990 EuroAssembler terminated with errorlevel 0.`

Expected output file t7121. bin

      0000: 43 31 43 32 43 33 43 34 43 35 43 36 43 37 0D 0A  C1C2C3C4C5C6C7·¬
      0010: 44 31 44 32 44 33 44 34 44 35 44 36 44 37 0D 0A  D1D2D3D4D5D6D7·¬
      0020: 45 31 45 32 45 33 45 34                          E1E2E3E4

▲Back to the top▲