| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5407: Machine instructions VFNMADD312SD VFNMADD123SD VFNMADD321SD VFNMSUB312SD VFNMSUB123SD VFNMSUB321SD

Tested procedures
  IibVFNMADD312SD IibVFNMADD123SD IibVFNMADD321SD IibVFNMSUB312SD IibVFNMSUB123SD IibVFNMSUB321SD

Source & expected listing t5407.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,DUMPALL=OFF,CPU=X64,SIMD=AVX512,FMA=ON,EVEX=ON | |t5407 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E2E99DCB | VFNMADD312SD XMM1,XMM2,XMM3 |00000005:62F2ED589DCB | VFNMADD312SD XMM1,XMM2,XMM3,ROUND=UP |0000000B:62F2ED8C9DCB | VFNMADD312SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000011:62F2ED8C9D4D08<3 | VFNMADD312SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000018:C4E2E9ADCB | VFNMADD123SD XMM1,XMM2,XMM3 |0000001D:62F2ED58ADCB | VFNMADD123SD XMM1,XMM2,XMM3,ROUND=UP |00000023:62F2ED8CADCB | VFNMADD123SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000029:62F2ED8CAD4D08<3 | VFNMADD123SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000030:C4E2E9BDCB | VFNMADD321SD XMM1,XMM2,XMM3 |00000035:62F2ED58BDCB | VFNMADD321SD XMM1,XMM2,XMM3,ROUND=UP |0000003B:62F2ED8CBDCB | VFNMADD321SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000041:62F2ED8CBD4D08<3 | VFNMADD321SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000048:C4E2E99FCB | VFNMSUB312SD XMM1,XMM2,XMM3 |0000004D:62F2ED589FCB | VFNMSUB312SD XMM1,XMM2,XMM3,ROUND=UP |00000053:62F2ED8C9FCB | VFNMSUB312SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000059:62F2ED8C9F4D08<3 | VFNMSUB312SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000060:C4E2E9AFCB | VFNMSUB123SD XMM1,XMM2,XMM3 |00000065:62F2ED58AFCB | VFNMSUB123SD XMM1,XMM2,XMM3,ROUND=UP |0000006B:62F2ED8CAFCB | VFNMSUB123SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000071:62F2ED8CAF4D08<3 | VFNMSUB123SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000078:C4E2E9BFCB | VFNMSUB321SD XMM1,XMM2,XMM3 |0000007D:62F2ED58BFCB | VFNMSUB321SD XMM1,XMM2,XMM3,ROUND=UP |00000083:62F2ED8CBFCB | VFNMSUB321SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000089:62F2ED8CBF4D08<3 | VFNMSUB321SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON | |ENDPROGRAM t5407`

Expected messages t5407.out
  `I0180 Assembling source file "t5407.htm". I0270 Assembling source "t5407". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5407". "t5407.htm"{64} I0510 Assembling program pass 1. "t5407.htm"{64} I0530 Assembling program pass 2 - final. "t5407.htm"{64} I0660 16bit TINY BIN file "t5407.bin" created, size=144. "t5407.htm"{90} I0650 Program "t5407" assembled in 2 passes with errorlevel 0. "t5407.htm"{90} I0750 Source "t5407" (108 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5407.htm.lst" created, size=2184. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲