| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3735: Machine instructions MOVUPS, MOVAPS

Tested procedures
  IipMOVUPS IipMOVAPS

Source & expected listing t3735.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64, SIMD=SSE | |t3735 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F10CF | MOVUPS XMM1,XMM7 |0003:0F10CF | MOVUPS XMM1,XMM7,CODE=SHORT |0006:0F11F9 | MOVUPS XMM1,XMM7,CODE=LONG |0009:0F100C | MOVUPS XMM1,[SI] |000C:0F110C | MOVUPS [SI],XMM1 |000F:0F100E0000 | MOVUPS XMM1,[0] |0014:0F113E0000 | MOVUPS [0],XMM7 |0019:0F28CF | MOVAPS XMM1,XMM7 |001C:0F28CF | MOVAPS XMM1,XMM7,CODE=SHORT |001F:0F29F9 | MOVAPS XMM1,XMM7,CODE=LONG |0022:0F280C | MOVAPS XMM1,[SI] |0025:0F290C | MOVAPS [SI],XMM1 |0028:0F280E0000 | MOVAPS XMM1,[0] |002D:0F293E0000 | MOVAPS [0],XMM7 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F10CF | MOVUPS XMM1,XMM7 |00000003:0F10CF | MOVUPS XMM1,XMM7,CODE=SHORT |00000006:0F11F9 | MOVUPS XMM1,XMM7,CODE=LONG |00000009:0F100E | MOVUPS XMM1,[ESI] |0000000C:0F110E | MOVUPS [ESI],XMM1 |0000000F:670F104C10 | MOVUPS XMM1,[SI+16] |00000014:670F117C10 | MOVUPS [SI+16],XMM7 |00000019:0F28CF | MOVAPS XMM1,XMM7 |0000001C:0F28CF | MOVAPS XMM1,XMM7,CODE=SHORT |0000001F:0F29F9 | MOVAPS XMM1,XMM7,CODE=LONG |00000022:0F280E | MOVAPS XMM1,[ESI] |00000025:0F290E | MOVAPS [ESI],XMM1 |00000028:0F280D00000000 | MOVAPS XMM1,[0] |0000002F:0F293D00000000 | MOVAPS [0],XMM7 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:410F10CB | MOVUPS XMM1,XMM11 |00000004:410F10CB | MOVUPS XMM1,XMM11,CODE=SHORT |00000008:440F11D9 | MOVUPS XMM1,XMM11,CODE=LONG |0000000C:440F101E | MOVUPS XMM11,[RSI] |00000010:440F111E | MOVUPS [RSI],XMM11 |00000014:440F101C2500000000 | MOVUPS XMM11,[0] |0000001D:440F111C2500000000 | MOVUPS [0],XMM11 |00000026:450F28D3 | MOVAPS XMM10,XMM11 |0000002A:450F28D3 | MOVAPS XMM10,XMM11,CODE=SHORT |0000002E:450F29DA | MOVAPS XMM10,XMM11,CODE=LONG |00000032:0F284E10 | MOVAPS XMM1,[RSI+16] |00000036:0F294E10 | MOVAPS [RSI+16],XMM1 |0000003A:67460F281C0E | MOVAPS XMM11,[ESI+R9D] |00000040:67460F291C0E | MOVAPS [ESI+R9D],XMM11 | |ENDPROGRAM t3735`

Expected messages t3735.out
  `I0180 Assembling source file "t3735.htm". I0270 Assembling source "t3735". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3735". "t3735.htm"{52} I0510 Assembling program pass 1. "t3735.htm"{52} I0530 Assembling program pass 2 - final. "t3735.htm"{52} I0660 16bit TINY BIN file "t3735.bin" created, size=198. "t3735.htm"{98} I0650 Program "t3735" assembled in 2 passes with errorlevel 0. "t3735.htm"{98} I0750 Source "t3735" (116 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3735.htm.lst" created, size=2661. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲