| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3800: Machine instructions PMOVZXBW PMOVZXBD PMOVZXBQ PMOVZXWD PMOVZXWQ PMOVZXDQ

Tested procedures
  IipGroupSSE4_1 IipPMOVZXBW IipPMOVZXBD IipPMOVZXBQ IipPMOVZXWD IipPMOVZXWQ IipPMOVZXDQ

Source & expected listing t3800.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=X64, SIMD=SSE4.1 | |t3800 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:660F3830CF | PMOVZXBW XMM1,XMM7 |0005:660F38300C | PMOVZXBW XMM1,[SI] |000A:660F3831CF | PMOVZXBD XMM1,XMM7 |000F:660F38310C | PMOVZXBD XMM1,[SI] |0014:660F3832CF | PMOVZXBQ XMM1,XMM7 |0019:660F38320C | PMOVZXBQ XMM1,[SI] |001E:660F3833CF | PMOVZXWD XMM1,XMM7 |0023:660F38330C | PMOVZXWD XMM1,[SI] |0028:660F3834CF | PMOVZXWQ XMM1,XMM7 |002D:660F38340C | PMOVZXWQ XMM1,[SI] |0032:660F3835CF | PMOVZXDQ XMM1,XMM7 |0037:660F38350C | PMOVZXDQ XMM1,[SI] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660F3830CF | PMOVZXBW XMM1,XMM7 |00000005:660F38300E | PMOVZXBW XMM1,[ESI] |0000000A:660F3831CF | PMOVZXBD XMM1,XMM7 |0000000F:660F38310E | PMOVZXBD XMM1,[ESI] |00000014:660F3832CF | PMOVZXBQ XMM1,XMM7 |00000019:660F38320E | PMOVZXBQ XMM1,[ESI] |0000001E:660F3833CF | PMOVZXWD XMM1,XMM7 |00000023:660F38330E | PMOVZXWD XMM1,[ESI] |00000028:660F3834CF | PMOVZXWQ XMM1,XMM7 |0000002D:660F38340E | PMOVZXWQ XMM1,[ESI] |00000032:660F3835CF | PMOVZXDQ XMM1,XMM7 |00000037:66670F38350C | PMOVZXDQ XMM1,[SI] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:66410F3830CB | PMOVZXBW XMM1,XMM11 |00000006:66450F3830CB | PMOVZXBW XMM9,XMM11 |0000000C:660F38300E | PMOVZXBW XMM1,[RSI] |00000011:660F3831CF | PMOVZXBD XMM1,XMM7 |00000016:66450F3831CB | PMOVZXBD XMM9,XMM11 |0000001C:66670F38310E | PMOVZXBD XMM1,[ESI] |00000022:660F3832CF | PMOVZXBQ XMM1,XMM7 |00000027:66440F3832CF | PMOVZXBQ XMM9,XMM7 |0000002D:6667420F38320C0E | PMOVZXBQ XMM1,[ESI+R9D] |00000035:660F3833CF | PMOVZXWD XMM1,XMM7 |0000003A:66450F3833CB | PMOVZXWD XMM9,XMM11 |00000040:660F38330C2500000000 | PMOVZXWD XMM1,[0] |0000004A:660F3834CF | PMOVZXWQ XMM1,XMM7 |0000004F:66440F38340E | PMOVZXWQ XMM9,[RSI] |00000055:660F3835CF | PMOVZXDQ XMM1,XMM7 |0000005A:66460F38355C4E10 | PMOVZXDQ XMM11,[RSI+2*R9+16] | |ENDPROGRAM t3800`

Expected messages t3800.out
  `I0180 Assembling source file "t3800.htm". I0270 Assembling source "t3800". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3800". "t3800.htm"{67} I0510 Assembling program pass 1. "t3800.htm"{67} I0530 Assembling program pass 2 - final. "t3800.htm"{67} I0660 16bit TINY BIN file "t3800.bin" created, size=226. "t3800.htm"{111} I0650 Program "t3800" assembled in 2 passes with errorlevel 0. "t3800.htm"{111} I0750 Source "t3800" (129 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3800.htm.lst" created, size=2601. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲