| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3560: Machine instructions FXCH FXCH4 FXCH7

Tested procedures
  IifFXCH IifFXCH7 IifFXCH4

Source & expected listing t3560.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=386,FPU=ON | |t3560 PROGRAM FORMAT=BIN, WIDTH=16, LISTMAP=OFF, LISTGLOBALS=OFF, |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:D9C9 | FXCH |00000002:D9C9 | FXCH ST1 |00000004:D9C9 | FXCH ST1,ST0 |00000006:D9C9 | FXCH ST0,ST1 |00000008:D9CF | FXCH ST7 |0000000A:D9CF | FXCH ST7,ST0 |0000000C:D9CF | FXCH ST0,ST7 |0000000E:D9C8 | FXCH ST0 |00000010:D9C8 | FXCH ST0,ST0 | |EUROASM UNDOC=ENABLE |00000012:DDC9 | FXCH4 |00000014:DDC9 | FXCH4 ST1 |00000016:DDC9 | FXCH4 ST1,ST0 |00000018:DDC9 | FXCH4 ST0,ST1 |0000001A:DDCF | FXCH4 ST7 |0000001C:DDCF | FXCH4 ST7,ST0 |0000001E:DDCF | FXCH4 ST0,ST7 |00000020:DDC8 | FXCH4 ST0 |00000022:DDC8 | FXCH4 ST0,ST0 |00000024:DFC9 | FXCH7 |00000026:DFC9 | FXCH7 ST1 |00000028:DFC9 | FXCH7 ST1,ST0 |0000002A:DFC9 | FXCH7 ST0,ST1 |0000002C:DFCF | FXCH7 ST7 |0000002E:DFCF | FXCH7 ST7,ST0 |00000030:DFCF | FXCH7 ST0,ST7 |00000032:DFC8 | FXCH7 ST0 |00000034:DFC8 | FXCH7 ST0,ST0 | |ENDPROGRAM t3560`

Expected messages t3560.out
  `I0180 Assembling source file "t3560.htm". I0270 Assembling source "t3560". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3560". "t3560.htm"{55} I0510 Assembling program pass 1. "t3560.htm"{55} I0530 Assembling program pass 2 - final. "t3560.htm"{55} I0660 16bit TINY BIN file "t3560.bin" created, size=54. "t3560.htm"{85} I0650 Program "t3560" assembled in 2 passes with errorlevel 0. "t3560.htm"{85} I0750 Source "t3560" (103 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3560.htm.lst" created, size=1332. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲