| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5734: Machine instructions VPANDN VPANDND VPANDNQ

Tested procedures
  IiyVPANDN IiyVPANDND IiyVPANDNQ

Source & expected listing t5734.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5734 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5E9DFCB | VPANDN XMM1,XMM2,XMM3 |00000004:C5EDDFCB | VPANDN YMM1,YMM2,YMM3 |00000008:C5E9DF4D40 | VPANDN XMM1,XMM2,[RBP+40h] |0000000D:C5EDDF4D40 | VPANDN YMM1,YMM2,[RBP+40h] |00000012:62F16D08DFCB | VPANDND XMM1,XMM2,XMM3 |00000018:62F16D28DFCB | VPANDND YMM1,YMM2,YMM3 |0000001E:62F16D8CDFCB | VPANDND XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000024:62F16DACDFCB | VPANDND YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000002A:62F16DCCDFCB | VPANDND ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000030:62F1692CDFCB | VPANDND ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=2 ; MVEX {badc}. |00000036:62F1694CDFCB | VPANDND ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=4 ; MVEX {aaaa}. |0000003C:62F16D08DF4D04<4 | VPANDND XMM1,XMM2,[RBP+40h],BCST=OFF |00000043:62F16D28DF4D02<5 | VPANDND YMM1,YMM2,[RBP+40h],BCST=OFF |0000004A:62F16D48DF4D01<6 | VPANDND ZMM1,ZMM2,[RBP+40h],BCST=OFF |00000051:62F16D18DF4D10<2 | VPANDND XMM1,XMM2,[RBP+40h],BCST=ON |00000058:62F16D38DF4D10<2 | VPANDND YMM1,YMM2,[RBP+40h],BCST=ON |0000005F:62F16D58DF4D10<2 | VPANDND ZMM1,ZMM2,[RBP+40h],BCST=ON |00000066:62F16908DF4D01<6 | VPANDND ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |0000006D:62F16918DF4D10<2 | VPANDND ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |00000074:62F16928DF4D04<4 | VPANDND ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |0000007B:62F1ED8CDFCB | VPANDNQ XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000081:62F1EDACDFCB | VPANDNQ YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000087:62F1EDCCDFCB | VPANDNQ ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |0000008D:62F1E92CDFCB | VPANDNQ ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=2 ; MVEX {badc}. |00000093:62F1E94CDFCB | VPANDNQ ZMM1,ZMM2,ZMM3,MASK=K4,EH=0,OPER=4 ; MVEX {aaaa}. |00000099:62F1ED8CDF4D04<4 | VPANDNQ XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=OFF |000000A0:62F1EDACDF4D02<5 | VPANDNQ YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=OFF |000000A7:62F1EDCCDF4D01<6 | VPANDNQ ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=OFF |000000AE:62F1ED9CDF4D08<3 | VPANDNQ XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000B5:62F1EDBCDF4D08<3 | VPANDNQ YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000BC:62F1EDDCDF4D08<3 | VPANDNQ ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000C3:62F1E908DF4D01<6 | VPANDNQ ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |000000CA:62F1E918DF4D08<3 | VPANDNQ ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |000000D1:62F1E928DF4D02<5 | VPANDNQ ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. | |ENDPROGRAM t5734`

Expected messages t5734.out
  `I0180 Assembling source file "t5734.htm". I0270 Assembling source "t5734". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5734". "t5734.htm"{55} I0510 Assembling program pass 1. "t5734.htm"{55} I0530 Assembling program pass 2 - final. "t5734.htm"{55} I0660 16bit TINY BIN file "t5734.bin" created, size=216. "t5734.htm"{91} I0650 Program "t5734" assembled in 2 passes with errorlevel 0. "t5734.htm"{91} I0750 Source "t5734" (109 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5734.htm.lst" created, size=2927. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲