| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5604: Machine instructions VPMINSB VPMINSW VPMINSD VPMINSQ

Tested procedures
  IizVPMINSB IizVPMINSW IizVPMINSD IizVPMINSQ

Source & expected listing t5604.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5604 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E26938CB | VPMINSB XMM1,XMM2,XMM3 |00000005:C4E26D38CB | VPMINSB YMM1,YMM2,YMM3 |0000000A:62F26D0C38CB | VPMINSB XMM1,XMM2,XMM3,MASK=K4 |00000010:62F26DAC38CB | VPMINSB YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000016:62F26DCC38CB | VPMINSB ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |0000001C:C4E269384D40 | VPMINSB XMM1,XMM2,[RBP+40h] |00000022:C4E26D384D40 | VPMINSB YMM1,YMM2,[RBP+40h] |00000028:62F26D48384D01<6 | VPMINSB ZMM1,ZMM2,[RBP+40h] |0000002F:62F26D0C384D04<4 | VPMINSB XMM1,XMM2,[RBP+40h],MASK=K4 |00000036:62F26DCC384D01<6 | VPMINSB ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000003D:C5E9EACB | VPMINSW XMM1,XMM2,XMM3 |00000041:C5EDEACB | VPMINSW YMM1,YMM2,YMM3 |00000045:62F16D0CEACB | VPMINSW XMM1,XMM2,XMM3,MASK=K4 |0000004B:62F16DACEACB | VPMINSW YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000051:62F16DCCEACB | VPMINSW ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000057:C5E9EA4D40 | VPMINSW XMM1,XMM2,[RBP+40h] |0000005C:C5EDEA4D40 | VPMINSW YMM1,YMM2,[RBP+40h] |00000061:62F16D48EA4D01<6 | VPMINSW ZMM1,ZMM2,[RBP+40h] |00000068:62F16D0CEA4D04<4 | VPMINSW XMM1,XMM2,[RBP+40h],MASK=K4 |0000006F:62F16DACEA4D02<5 | VPMINSW YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000076:62F16DCCEA4D01<6 | VPMINSW ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000007D:C4E26939CB | VPMINSD XMM1,XMM2,XMM3 |00000082:C4E26D39CB | VPMINSD YMM1,YMM2,YMM3 |00000087:62F26D0C39CB | VPMINSD XMM1,XMM2,XMM3,MASK=K4 |0000008D:62F26DAC39CB | VPMINSD YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000093:62F26DCC39CB | VPMINSD ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000099:62F2692839CB | VPMINSD ZMM1,ZMM2,ZMM3,EH=0,OPER=2 ; MVEX swizzle {badc}. |0000009F:C4E269394D40 | VPMINSD XMM1,XMM2,[RBP+40h] |000000A5:C4E26D394D40 | VPMINSD YMM1,YMM2,[RBP+40h] |000000AB:62F26D48394D01<6 | VPMINSD ZMM1,ZMM2,[RBP+40h] |000000B2:62F26D18394D10<2 | VPMINSD XMM1,XMM2,[RBP+40h],BCST=ON |000000B9:62F26D38394D10<2 | VPMINSD YMM1,YMM2,[RBP+40h],BCST=ON |000000C0:62F26D58394D10<2 | VPMINSD ZMM1,ZMM2,[RBP+40h],BCST=ON |000000C7:62F26D0C394D04<4 | VPMINSD XMM1,XMM2,[RBP+40h],MASK=K4 |000000CE:62F26D1C394D10<2 | VPMINSD XMM1,XMM2,[RBP+40h],MASK=K4,BCST=ON |000000D5:62F26DBC394D10<2 | VPMINSD YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000DC:62F26DCC394D01<6 | VPMINSD ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000E3:62F26908394D01<6 | VPMINSD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |000000EA:62F26918394D10<2 | VPMINSD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |000000F1:62F26928394D04<4 | VPMINSD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |000000F8:62F26948394D04<4 | VPMINSD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |000000FF:62F2ED0839CB | VPMINSQ XMM1,XMM2,XMM3 |00000105:62F2EDAC39CB | VPMINSQ YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000010B:62F2EDCC39CB | VPMINSQ ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000111:62F2ED08394D04<4 | VPMINSQ XMM1,XMM2,[RBP+40h] |00000118:62F2ED28394D02<5 | VPMINSQ YMM1,YMM2,[RBP+40h] |0000011F:62F2ED48394D01<6 | VPMINSQ ZMM1,ZMM2,[RBP+40h] |00000126:62F2ED18394D08<3 | VPMINSQ XMM1,XMM2,[RBP+40h],BCST=ON |0000012D:62F2ED38394D08<3 | VPMINSQ YMM1,YMM2,[RBP+40h],BCST=ON |00000134:62F2ED58394D08<3 | VPMINSQ ZMM1,ZMM2,[RBP+40h],BCST=ON |0000013B:62F2ED0C394D04<4 | VPMINSQ XMM1,XMM2,[RBP+40h],MASK=K4 |00000142:62F2ED1C394D08<3 | VPMINSQ XMM1,XMM2,[RBP+40h],MASK=K4,BCST=ON |00000149:62F2EDBC394D08<3 | VPMINSQ YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |00000150:62F2EDCC394D01<6 | VPMINSQ ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON | |ENDPROGRAM t5604`

Expected messages t5604.out
  `I0180 Assembling source file "t5604.htm". I0270 Assembling source "t5604". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5604". "t5604.htm"{58} I0510 Assembling program pass 1. "t5604.htm"{58} I0530 Assembling program pass 2 - final. "t5604.htm"{58} I0660 16bit TINY BIN file "t5604.bin" created, size=343. "t5604.htm"{114} I0650 Program "t5604" assembled in 2 passes with errorlevel 0. "t5604.htm"{114} I0750 Source "t5604" (132 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5604.htm.lst" created, size=4046. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲