| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3114: Machine instructions AND ANDB ANDW ANDD in 32bit mode

Tested procedures
  IigAND IigANDB IigANDW IigANDD

Source & expected listing t3114.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3114 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:2402 | AND AL,2 |00000002:80E002 | AND AL,2,CODE=LONG |00000005:66250200 | AND AX,2 |00000009:6683E002 | AND AX,2,CODE=LONG |0000000D:83E002 | AND EAX,2 |00000010:2502000000 | AND EAX,2,CODE=SHORT |00000015:80E102 | AND CL,2 |00000018:8025[AE000000]02 | AND [MemByte],2 |0000001F:6683E102 | AND CX,2 |00000023:6681E10200 | AND CX,2,IMM=WORD |00000028:668325[AC000000]02 | AND [MemWord],2 |00000030:668125[AC000000]0200 | AND [MemWord],2,IMM=WORD |00000039:8125[AC000000]02000000 | ANDD [MemWord],2,IMM=DWORD |00000043:83E102 | AND ECX,2 |00000046:81E102000000 | AND ECX,2,IMM=DWORD |0000004C:8325[A8000000]02 | AND [MemDword],2 |00000053:668325[A8000000]02 | ANDW [MemDword],2 |0000005B:8125[A8000000]02000000 | AND [MemDword],2,IMM=DWORD |00000065:802702 | ANDB [EDI],2 |00000068:66832702 | ANDW [EDI],2 |0000006C:832702 | ANDD [EDI],2 |0000006F:20D1 | AND CL,DL |00000071:22CA | AND CL,DL,CODE=LONG |00000073:20F5 | AND CH,DH |00000075:22EE | AND CH,DH,CODE=LONG |00000077:6621D1 | AND CX,DX |0000007A:6623CA | AND CX,DX,CODE=LONG |0000007D:21D1 | AND ECX,EDX |0000007F:23CA | AND ECX,EDX,CODE=LONG |00000081:220D[AE000000] | AND CL,[MemByte] |00000087:66230D[AC000000] | AND CX,[MemWord] |0000008E:230D[A8000000] | AND ECX,[MemDword] |00000094:2015[AE000000] | AND [MemByte],DL |0000009A:662115[AC000000] | AND [MemWord],DX |000000A1:2115[A8000000] | AND [MemDword],EDX |000000A7:90 | ALIGN QWORD |000000A8:00000000 |MemDword D D |000000AC:0000 |MemWord D W |000000AE:00 |MemByte D B | |ENDPROGRAM t3114`

Expected messages t3114.out
  `I0180 Assembling source file "t3114.htm". I0270 Assembling source "t3114". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3114". "t3114.htm"{58} I0510 Assembling program pass 1. "t3114.htm"{58} I0510 Assembling program pass 2. "t3114.htm"{58} I0510 Assembling program pass 3. "t3114.htm"{58} I0530 Assembling program pass 4 - final. "t3114.htm"{58} I0660 16bit TINY BIN file "t3114.bin" created, size=175. "t3114.htm"{99} I0650 Program "t3114" assembled in 4 passes with errorlevel 0. "t3114.htm"{99} I0750 Source "t3114" (119 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3114.htm.lst" created, size=2413. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲