| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3640: Machine instructions PSUBB PSUBW PSUBD PSUBQ PADDB PADDW PADDD

Tested procedures
  IimGroupSSE2 IimPSUBB IimPSUBW IimPSUBD IimPSUBQ IimPADDB IimPADDW IimPADDD

Source & expected listing t3640.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64, MMX=ON, SIMD=SSE2 | |t3640 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0FF8CF | PSUBB MM1,MM7 |0003:260FF814 | PSUBB MM2,[ES:SI] |0007:660FF8CF | PSUBB XMM1,XMM7 |000B:660FF856F8 | PSUBB XMM2,[BP-8] |0010:0FF9CF | PSUBW MM1,MM7 |0013:260FF914 | PSUBW MM2,[ES:SI] |0017:660FF9CF | PSUBW XMM1,XMM7 |001B:660FF956F8 | PSUBW XMM2,[BP-8] |0020:0FFACF | PSUBD MM1,MM7 |0023:260FFA14 | PSUBD MM2,[ES:SI] |0027:660FFACF | PSUBD XMM1,XMM7 |002B:660FFA56F8 | PSUBD XMM2,[BP-8] |0030:0FFBCF | PSUBQ MM1,MM7 |0033:260FFB14 | PSUBQ MM2,[ES:SI] |0037:660FFBCF | PSUBQ XMM1,XMM7 |003B:660FFB56F8 | PSUBQ XMM2,[BP-8] |0040:0FFCCF | PADDB MM1,MM7 |0043:260FFC14 | PADDB MM2,[ES:SI] |0047:660FFCCF | PADDB XMM1,XMM7 |004B:660FFC56F8 | PADDB XMM2,[BP-8] |0050:0FFDCF | PADDW MM1,MM7 |0053:260FFD14 | PADDW MM2,[ES:SI] |0057:660FFDCF | PADDW XMM1,XMM7 |005B:660FFD56F8 | PADDW XMM2,[BP-8] |0060:0FFECF | PADDD MM1,MM7 |0063:260FFE14 | PADDD MM2,[ES:SI] |0067:660FFECF | PADDD XMM1,XMM7 |006B:660FFE56F8 | PADDD XMM2,[BP-8] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0FF8CF | PSUBB MM1,MM7 |00000003:0FF816 | PSUBB MM2,[ESI] |00000006:660FF8CF | PSUBB XMM1,XMM7 |0000000A:66670FF856F8 | PSUBB XMM2,[BP-8] |00000010:0FF9CF | PSUBW MM1,MM7 |00000013:0FF916 | PSUBW MM2,[ESI] |00000016:660FF9CF | PSUBW XMM1,XMM7 |0000001A:66670FF956F8 | PSUBW XMM2,[BP-8] |00000020:0FFACF | PSUBD MM1,MM7 |00000023:0FFA16 | PSUBD MM2,[ESI] |00000026:660FFACF | PSUBD XMM1,XMM7 |0000002A:66670FFA56F8 | PSUBD XMM2,[BP-8] |00000030:0FFBCF | PSUBQ MM1,MM7 |00000033:0FFB16 | PSUBQ MM2,[ESI] |00000036:660FFBCF | PSUBQ XMM1,XMM7 |0000003A:66670FFB56F8 | PSUBQ XMM2,[BP-8] |00000040:0FFCCF | PADDB MM1,MM7 |00000043:0FFC16 | PADDB MM2,[ESI] |00000046:660FFCCF | PADDB XMM1,XMM7 |0000004A:66670FFC56F8 | PADDB XMM2,[BP-8] |00000050:0FFDCF | PADDW MM1,MM7 |00000053:0FFD16 | PADDW MM2,[ESI] |00000056:660FFDCF | PADDW XMM1,XMM7 |0000005A:66670FFD56F8 | PADDW XMM2,[BP-8] |00000060:0FFECF | PADDD MM1,MM7 |00000063:0FFE16 | PADDD MM2,[ESI] |00000066:660FFECF | PADDD XMM1,XMM7 |0000006A:66670FFE56F8 | PADDD XMM2,[BP-8] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0FF8CF | PSUBB MM1,MM7 |00000003:670FF816 | PSUBB MM2,[ESI] |00000007:660FF8CF | PSUBB XMM1,XMM7 |0000000B:66410FF8542DF8 | PSUBB XMM2,[R13+RBP-8] |00000012:0FF9CF | PSUBW MM1,MM7 |00000015:670FF916 | PSUBW MM2,[ESI] |00000019:660FF9CF | PSUBW XMM1,XMM7 |0000001D:66410FF9542DF8 | PSUBW XMM2,[R13+RBP-8] |00000024:0FFACF | PSUBD MM1,MM7 |00000027:670FFA16 | PSUBD MM2,[ESI] |0000002B:660FFACF | PSUBD XMM1,XMM7 |0000002F:66410FFA542DF8 | PSUBD XMM2,[R13+RBP-8] |00000036:0FFBCF | PSUBQ MM1,MM7 |00000039:670FFB16 | PSUBQ MM2,[ESI] |0000003D:660FFBCF | PSUBQ XMM1,XMM7 |00000041:66410FFB542DF8 | PSUBQ XMM2,[R13+RBP-8] |00000048:0FFCCF | PADDB MM1,MM7 |0000004B:670FFC16 | PADDB MM2,[ESI] |0000004F:660FFCCF | PADDB XMM1,XMM7 |00000053:66410FFC542DF8 | PADDB XMM2,[R13+RBP-8] |0000005A:0FFDCF | PADDW MM1,MM7 |0000005D:670FFD16 | PADDW MM2,[ESI] |00000061:660FFDCF | PADDW XMM1,XMM7 |00000065:66410FFD542DF8 | PADDW XMM2,[R13+RBP-8] |0000006C:0FFECF | PADDD MM1,MM7 |0000006F:670FFE16 | PADDD MM2,[ESI] |00000073:660FFECF | PADDD XMM1,XMM7 |00000077:66410FFE542DF8 | PADDD XMM2,[R13+RBP-8] | |ENDPROGRAM t3640`

Expected messages t3640.out
  `I0180 Assembling source file "t3640.htm". I0270 Assembling source "t3640". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3640". "t3640.htm"{70} I0510 Assembling program pass 1. "t3640.htm"{70} I0530 Assembling program pass 2 - final. "t3640.htm"{70} I0660 16bit TINY BIN file "t3640.bin" created, size=350. "t3640.htm"{158} I0650 Program "t3640" assembled in 2 passes with errorlevel 0. "t3640.htm"{158} I0750 Source "t3640" (176 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3640.htm.lst" created, size=4537. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲