| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3620: Machine instructions PUNPCKHBW PUNPCKHWD PUNPCKHDQ PACKSSDW PCMPEQB PCMPEQW PCMPEQD PADDQ

Tested procedures
  IimGroupSSE2 IimPUNPCKHBW IimPUNPCKHWD IimPUNPCKHDQ IimPACKSSDW IimPCMPEQB IimPCMPEQW IimPCMPEQD IimPADDQ

Source & expected listing t3620.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64, MMX=ON, SIMD=SSE2 | |t3620 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F68CF | PUNPCKHBW MM1,MM7 |0003:260F6814 | PUNPCKHBW MM2,[ES:SI] |0007:660F68CF | PUNPCKHBW XMM1,XMM7 |000B:660F6856F8 | PUNPCKHBW XMM2,[BP-8] |0010:0F69CF | PUNPCKHWD MM1,MM7 |0013:260F6914 | PUNPCKHWD MM2,[ES:SI] |0017:660F69CF | PUNPCKHWD XMM1,XMM7 |001B:660F6956F8 | PUNPCKHWD XMM2,[BP-8] |0020:0F6ACF | PUNPCKHDQ MM1,MM7 |0023:260F6A14 | PUNPCKHDQ MM2,[ES:SI] |0027:660F6ACF | PUNPCKHDQ XMM1,XMM7 |002B:660F6A56F8 | PUNPCKHDQ XMM2,[BP-8] |0030:0F6BCF | PACKSSDW MM1,MM7 |0033:260F6B14 | PACKSSDW MM2,[ES:SI] |0037:660F6BCF | PACKSSDW XMM1,XMM7 |003B:660F6B56F8 | PACKSSDW XMM2,[BP-8] |0040:0F74CF | PCMPEQB MM1,MM7 |0043:260F7414 | PCMPEQB MM2,[ES:SI] |0047:660F74CF | PCMPEQB XMM1,XMM7 |004B:660F7456F8 | PCMPEQB XMM2,[BP-8] |0050:0F75CF | PCMPEQW MM1,MM7 |0053:260F7514 | PCMPEQW MM2,[ES:SI] |0057:660F75CF | PCMPEQW XMM1,XMM7 |005B:660F7556F8 | PCMPEQW XMM2,[BP-8] |0060:0F76CF | PCMPEQD MM1,MM7 |0063:260F7614 | PCMPEQD MM2,[ES:SI] |0067:660F76CF | PCMPEQD XMM1,XMM7 |006B:660F7656F8 | PCMPEQD XMM2,[BP-8] |0070:0FD4CF | PADDQ MM1,MM7 |0073:260FD414 | PADDQ MM2,[ES:SI] |0077:660FD4CF | PADDQ XMM1,XMM7 |007B:660FD456F8 | PADDQ XMM2,[BP-8] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F68CF | PUNPCKHBW MM1,MM7 |00000003:0F6816 | PUNPCKHBW MM2,[ESI] |00000006:660F68CF | PUNPCKHBW XMM1,XMM7 |0000000A:66670F6856F8 | PUNPCKHBW XMM2,[BP-8] |00000010:0F69CF | PUNPCKHWD MM1,MM7 |00000013:0F6916 | PUNPCKHWD MM2,[ESI] |00000016:660F69CF | PUNPCKHWD XMM1,XMM7 |0000001A:66670F6956F8 | PUNPCKHWD XMM2,[BP-8] |00000020:0F6ACF | PUNPCKHDQ MM1,MM7 |00000023:0F6A16 | PUNPCKHDQ MM2,[ESI] |00000026:660F6ACF | PUNPCKHDQ XMM1,XMM7 |0000002A:66670F6A56F8 | PUNPCKHDQ XMM2,[BP-8] |00000030:0F6BCF | PACKSSDW MM1,MM7 |00000033:0F6B16 | PACKSSDW MM2,[ESI] |00000036:660F6BCF | PACKSSDW XMM1,XMM7 |0000003A:66670F6B56F8 | PACKSSDW XMM2,[BP-8] |00000040:0F74CF | PCMPEQB MM1,MM7 |00000043:0F7416 | PCMPEQB MM2,[ESI] |00000046:660F74CF | PCMPEQB XMM1,XMM7 |0000004A:66670F7456F8 | PCMPEQB XMM2,[BP-8] |00000050:0F75CF | PCMPEQW MM1,MM7 |00000053:0F7516 | PCMPEQW MM2,[ESI] |00000056:660F75CF | PCMPEQW XMM1,XMM7 |0000005A:66670F7556F8 | PCMPEQW XMM2,[BP-8] |00000060:0F76CF | PCMPEQD MM1,MM7 |00000063:0F7616 | PCMPEQD MM2,[ESI] |00000066:660F76CF | PCMPEQD XMM1,XMM7 |0000006A:66670F7656F8 | PCMPEQD XMM2,[BP-8] |00000070:0FD4CF | PADDQ MM1,MM7 |00000073:0FD416 | PADDQ MM2,[ESI] |00000076:660FD4CF | PADDQ XMM1,XMM7 |0000007A:66670FD456F8 | PADDQ XMM2,[BP-8] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0F68CF | PUNPCKHBW MM1,MM7 |00000003:670F6816 | PUNPCKHBW MM2,[ESI] |00000007:660F68CF | PUNPCKHBW XMM1,XMM7 |0000000B:66410F68542DF8 | PUNPCKHBW XMM2,[R13+RBP-8] |00000012:0F69CF | PUNPCKHWD MM1,MM7 |00000015:670F6916 | PUNPCKHWD MM2,[ESI] |00000019:660F69CF | PUNPCKHWD XMM1,XMM7 |0000001D:66410F69542DF8 | PUNPCKHWD XMM2,[R13+RBP-8] |00000024:0F6ACF | PUNPCKHDQ MM1,MM7 |00000027:670F6A16 | PUNPCKHDQ MM2,[ESI] |0000002B:660F6ACF | PUNPCKHDQ XMM1,XMM7 |0000002F:66410F6A542DF8 | PUNPCKHDQ XMM2,[R13+RBP-8] |00000036:0F6BCF | PACKSSDW MM1,MM7 |00000039:670F6B16 | PACKSSDW MM2,[ESI] |0000003D:660F6BCF | PACKSSDW XMM1,XMM7 |00000041:66410F6B542DF8 | PACKSSDW XMM2,[R13+RBP-8] |00000048:0F74CF | PCMPEQB MM1,MM7 |0000004B:670F7416 | PCMPEQB MM2,[ESI] |0000004F:660F74CF | PCMPEQB XMM1,XMM7 |00000053:66410F74542DF8 | PCMPEQB XMM2,[R13+RBP-8] |0000005A:0F75CF | PCMPEQW MM1,MM7 |0000005D:670F7516 | PCMPEQW MM2,[ESI] |00000061:660F75CF | PCMPEQW XMM1,XMM7 |00000065:66410F75542DF8 | PCMPEQW XMM2,[R13+RBP-8] |0000006C:0F76CF | PCMPEQD MM1,MM7 |0000006F:670F7616 | PCMPEQD MM2,[ESI] |00000073:660F76CF | PCMPEQD XMM1,XMM7 |00000077:66410F76542DF8 | PCMPEQD XMM2,[R13+RBP-8] |0000007E:0FD4CF | PADDQ MM1,MM7 |00000081:670FD416 | PADDQ MM2,[ESI] |00000085:660FD4CF | PADDQ XMM1,XMM7 |00000089:66410FD4542DF8 | PADDQ XMM2,[R13+RBP-8] | |ENDPROGRAM t3620`

Expected messages t3620.out
  `I0180 Assembling source file "t3620.htm". I0270 Assembling source "t3620". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3620". "t3620.htm"{73} I0510 Assembling program pass 1. "t3620.htm"{73} I0530 Assembling program pass 2 - final. "t3620.htm"{73} I0660 16bit TINY BIN file "t3620.bin" created, size=400. "t3620.htm"{173} I0650 Program "t3620" assembled in 2 passes with errorlevel 0. "t3620.htm"{173} I0750 Source "t3620" (191 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3620.htm.lst" created, size=5377. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲