| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3625: Machine instructions PMULLW PSUBUSB PSUBUSW PMINUB PAND PADDUSB PADDUSW PMAXUB

Tested procedures
  IimGroupSSE2 IimPMULLW IimPSUBUSB IimPSUBUSW IimPMINUB IimPAND IimPADDUSB IimPADDUSW IimPMAXUB

Source & expected listing t3625.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64, MMX=ON, SIMD=SSE2 | |t3625 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0FD5CF | PMULLW MM1,MM7 |0003:260FD514 | PMULLW MM2,[ES:SI] |0007:660FD5CF | PMULLW XMM1,XMM7 |000B:660FD556F8 | PMULLW XMM2,[BP-8] |0010:0FD8CF | PSUBUSB MM1,MM7 |0013:260FD814 | PSUBUSB MM2,[ES:SI] |0017:660FD8CF | PSUBUSB XMM1,XMM7 |001B:660FD856F8 | PSUBUSB XMM2,[BP-8] |0020:0FD9CF | PSUBUSW MM1,MM7 |0023:260FD914 | PSUBUSW MM2,[ES:SI] |0027:660FD9CF | PSUBUSW XMM1,XMM7 |002B:660FD956F8 | PSUBUSW XMM2,[BP-8] |0030:0FDACF | PMINUB MM1,MM7 |0033:260FDA14 | PMINUB MM2,[ES:SI] |0037:660FDACF | PMINUB XMM1,XMM7 |003B:660FDA56F8 | PMINUB XMM2,[BP-8] |0040:0FDBCF | PAND MM1,MM7 |0043:260FDB14 | PAND MM2,[ES:SI] |0047:660FDBCF | PAND XMM1,XMM7 |004B:660FDB56F8 | PAND XMM2,[BP-8] |0050:0FDCCF | PADDUSB MM1,MM7 |0053:260FDC14 | PADDUSB MM2,[ES:SI] |0057:660FDCCF | PADDUSB XMM1,XMM7 |005B:660FDC56F8 | PADDUSB XMM2,[BP-8] |0060:0FDDCF | PADDUSW MM1,MM7 |0063:260FDD14 | PADDUSW MM2,[ES:SI] |0067:660FDDCF | PADDUSW XMM1,XMM7 |006B:660FDD56F8 | PADDUSW XMM2,[BP-8] |0070:0FDECF | PMAXUB MM1,MM7 |0073:260FDE14 | PMAXUB MM2,[ES:SI] |0077:660FDECF | PMAXUB XMM1,XMM7 |007B:660FDE56F8 | PMAXUB XMM2,[BP-8] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0FD5CF | PMULLW MM1,MM7 |00000003:0FD516 | PMULLW MM2,[ESI] |00000006:660FD5CF | PMULLW XMM1,XMM7 |0000000A:66670FD556F8 | PMULLW XMM2,[BP-8] |00000010:0FD8CF | PSUBUSB MM1,MM7 |00000013:0FD816 | PSUBUSB MM2,[ESI] |00000016:660FD8CF | PSUBUSB XMM1,XMM7 |0000001A:66670FD856F8 | PSUBUSB XMM2,[BP-8] |00000020:0FD9CF | PSUBUSW MM1,MM7 |00000023:0FD916 | PSUBUSW MM2,[ESI] |00000026:660FD9CF | PSUBUSW XMM1,XMM7 |0000002A:66670FD956F8 | PSUBUSW XMM2,[BP-8] |00000030:0FDACF | PMINUB MM1,MM7 |00000033:0FDA16 | PMINUB MM2,[ESI] |00000036:660FDACF | PMINUB XMM1,XMM7 |0000003A:66670FDA56F8 | PMINUB XMM2,[BP-8] |00000040:0FDBCF | PAND MM1,MM7 |00000043:0FDB16 | PAND MM2,[ESI] |00000046:660FDBCF | PAND XMM1,XMM7 |0000004A:66670FDB56F8 | PAND XMM2,[BP-8] |00000050:0FDCCF | PADDUSB MM1,MM7 |00000053:0FDC16 | PADDUSB MM2,[ESI] |00000056:660FDCCF | PADDUSB XMM1,XMM7 |0000005A:66670FDC56F8 | PADDUSB XMM2,[BP-8] |00000060:0FDDCF | PADDUSW MM1,MM7 |00000063:0FDD16 | PADDUSW MM2,[ESI] |00000066:660FDDCF | PADDUSW XMM1,XMM7 |0000006A:66670FDD56F8 | PADDUSW XMM2,[BP-8] |00000070:0FDECF | PMAXUB MM1,MM7 |00000073:0FDE16 | PMAXUB MM2,[ESI] |00000076:660FDECF | PMAXUB XMM1,XMM7 |0000007A:66670FDE56F8 | PMAXUB XMM2,[BP-8] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0FD5CF | PMULLW MM1,MM7 |00000003:670FD516 | PMULLW MM2,[ESI] |00000007:660FD5CF | PMULLW XMM1,XMM7 |0000000B:66410FD5542DF8 | PMULLW XMM2,[R13+RBP-8] |00000012:0FD8CF | PSUBUSB MM1,MM7 |00000015:670FD816 | PSUBUSB MM2,[ESI] |00000019:660FD8CF | PSUBUSB XMM1,XMM7 |0000001D:66410FD8542DF8 | PSUBUSB XMM2,[R13+RBP-8] |00000024:0FD9CF | PSUBUSW MM1,MM7 |00000027:670FD916 | PSUBUSW MM2,[ESI] |0000002B:660FD9CF | PSUBUSW XMM1,XMM7 |0000002F:66410FD9542DF8 | PSUBUSW XMM2,[R13+RBP-8] |00000036:0FDACF | PMINUB MM1,MM7 |00000039:670FDA16 | PMINUB MM2,[ESI] |0000003D:660FDACF | PMINUB XMM1,XMM7 |00000041:66410FDA542DF8 | PMINUB XMM2,[R13+RBP-8] |00000048:0FDBCF | PAND MM1,MM7 |0000004B:670FDB16 | PAND MM2,[ESI] |0000004F:660FDBCF | PAND XMM1,XMM7 |00000053:66410FDB542DF8 | PAND XMM2,[R13+RBP-8] |0000005A:0FDCCF | PADDUSB MM1,MM7 |0000005D:670FDC16 | PADDUSB MM2,[ESI] |00000061:660FDCCF | PADDUSB XMM1,XMM7 |00000065:66410FDC542DF8 | PADDUSB XMM2,[R13+RBP-8] |0000006C:0FDDCF | PADDUSW MM1,MM7 |0000006F:670FDD16 | PADDUSW MM2,[ESI] |00000073:660FDDCF | PADDUSW XMM1,XMM7 |00000077:66410FDD542DF8 | PADDUSW XMM2,[R13+RBP-8] |0000007E:0FDECF | PMAXUB MM1,MM7 |00000081:670FDE16 | PMAXUB MM2,[ESI] |00000085:660FDECF | PMAXUB XMM1,XMM7 |00000089:66410FDE542DF8 | PMAXUB XMM2,[R13+RBP-8] | |ENDPROGRAM t3625`

Expected messages t3625.out
  `I0180 Assembling source file "t3625.htm". I0270 Assembling source "t3625". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3625". "t3625.htm"{73} I0510 Assembling program pass 1. "t3625.htm"{73} I0530 Assembling program pass 2 - final. "t3625.htm"{73} I0660 16bit TINY BIN file "t3625.bin" created, size=400. "t3625.htm"{173} I0650 Program "t3625" assembled in 2 passes with errorlevel 0. "t3625.htm"{173} I0750 Source "t3625" (191 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3625.htm.lst" created, size=5245. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲