| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3333: Machine instructions BT BTW BTD BTQ

Tested procedures
  IigBT IigBTW IigBTD IigBTQ

Source & expected listing t3333.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,CPU=X64 | |t3333 PROGRAM FORMAT=BIN,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0FA3D1 | BT CX,DX |0003:660FA3D1 | BT ECX,EDX |0007:0FA314 | BT [SI],DX |000A:660FA314 | BT [SI],EDX |000E:0FA316[7C00] | BT [MemWord],DX |0013:660FA316[7800] | BT [MemDword],EDX |0019:0FBAE102 | BT CX,2 |001D:660FBAE102 | BT ECX,2 |0022:0FBA26[7C00]02 | BT [MemWord],2 |0028:660FBA26[7800]02 | BT [MemDword],2 |002F:0FBA2402 | BTW [SI],2 |0033:660FBA2402 | BTD [SI],2 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660FA3D1 | BT CX,DX |00000004:0FA3D1 | BT ECX,EDX |00000007:660FA316 | BT [ESI],DX |0000000B:0FA316 | BT [ESI],EDX |0000000E:660FA315[7C000000] | BT [MemWord],DX |00000016:0FA315[78000000] | BT [MemDword],EDX |0000001D:660FBAE102 | BT CX,2 |00000022:0FBAE102 | BT ECX,2 |00000026:660FBA25[7C000000]02 | BT [MemWord],2 |0000002F:0FBA25[78000000]02 | BT [MemDword],2 |00000037:660FBA2602 | BTW [ESI],2 |0000003C:0FBA2602 | BTD [ESI],2 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:660FA3D1 | BT CX,DX |00000004:0FA3D1 | BT ECX,EDX |00000007:480FA3D1 | BT RCX,RDX |0000000B:4D0FA3D1 | BT R9,R10 |0000000F:660FA316 | BT [RSI],DX |00000013:0FA316 | BT [RSI],EDX |00000016:480FA316 | BT [RSI],RDX |0000001A:660FA3155A000000 | BT [MemWord],DX |00000022:0FA3154F000000 | BT [MemDword],EDX |00000029:480FA3153F000000 | BT [MemQword],RDX |00000031:660FBAE102 | BT CX,2 |00000036:0FBAE102 | BT ECX,2 |0000003A:480FBAE102 | BT RCX,2 |0000003F:490FBAE102 | BT R9,2 |00000044:660FBA252F00000002 | BT [MemWord],2 |0000004D:0FBA252300000002 | BT [MemDword],2 |00000055:480FBA251200000002 | BT [MemQword],2 |0000005E:660FBA2602 | BTW [RSI],2 |00000063:0FBA2602 | BTD [RSI],2 |00000067:480FBA2602 | BTQ [RSI],2 |0000006C:0F1F4000 | ALIGN QWORD |00000070:0000000000000000 |MemQword DQ Q |00000078:00000000 |MemDword DD D |0000007C:0000 |MemWord DW W | |ENDPROGRAM t3333`

Expected messages t3333.out
  `I0180 Assembling source file "t3333.htm". I0270 Assembling source "t3333". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3333". "t3333.htm"{58} I0510 Assembling program pass 1. "t3333.htm"{58} I0510 Assembling program pass 2. "t3333.htm"{58} I0510 Assembling program pass 3. "t3333.htm"{58} I0530 Assembling program pass 4 - final. "t3333.htm"{58} I0660 16bit TINY BIN file "t3333.bin" created, size=254. "t3333.htm"{110} I0650 Program "t3333" assembled in 4 passes with errorlevel 0. "t3333.htm"{110} I0750 Source "t3333" (130 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3333.htm.lst" created, size=2768. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲