| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5444: Machine instructions VGATHERPF0DPS VGATHERPF0HINTDPS VGATHERPF0QPS VGATHERPF0DPD VGATHERPF0HINTDPD VGATHERPF0QPD

Tested procedures
  IizVGATHERPF0DPS IizVGATHERPF0HINTDPS IizVGATHERPF0QPS IizVGATHERPF0DPD IizVGATHERPF0HINTDPD IizVGATHERPF0QPD

Source & expected listing t5444.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,DUMPALL=OFF,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5444 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F27D4AC74C0D10<2 | VGATHERPF0QPS [ZMM1+RBP+40h],MASK=K2 |00000008:62F2FD4AC74C0D08<3 | VGATHERPF0QPD [ZMM1+RBP+40h],MASK=K2 |00000010:62F2FD4AC64C0D08<3 | VGATHERPF0DPD [YMM1+RBP+40h],MASK=K2 |00000018:62F27D4AC64C0D10<2 | VGATHERPF0DPS [ZMM1+RBP+40h],MASK=K2 |00000020:62F2790AC64C0D10<2 | VGATHERPF0DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=0 ; No conversion. |00000028:62F2793AC64C0D20<1 | VGATHERPF0DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=3 ; {float16}. |00000030:62F2794AC64C0D40 | VGATHERPF0DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=4 ; {uint8}. |00000038:62F2795AC64C0D40 | VGATHERPF0DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=5 ; {sint8}. |00000040:62F2796AC64C0D20<1 | VGATHERPF0DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=6 ; {uint16}. |00000048:62F2797AC64C0D20<1 | VGATHERPF0DPS [ZMM1+RBP+40h],MASK=K2,PREFIX=MVEX,OPER=7 ; {sint16}. |00000050:62F2F90AC6440D08<3 | VGATHERPF0HINTDPD [ZMM1+RBP+40h],MASK=K2 ; MVEX, no conversion. |00000058:62F2790AC6440D10<2 | VGATHERPF0HINTDPS [ZMM1+RBP+40h],MASK=K2,OPER=0 ; MVEX, no conversion. |00000060:62F2793AC6440D20<1 | VGATHERPF0HINTDPS [ZMM1+RBP+40h],MASK=K2,OPER=3 ; {float16}. |00000068:62F2794AC6440D40 | VGATHERPF0HINTDPS [ZMM1+RBP+40h],MASK=K2,OPER=4 ; {uint8}. |00000070:62F2795AC6440D40 | VGATHERPF0HINTDPS [ZMM1+RBP+40h],MASK=K2,OPER=5 ; {sint8}. |00000078:62F2796AC6440D20<1 | VGATHERPF0HINTDPS [ZMM1+RBP+40h],MASK=K2,OPER=6 ; {uint16}. |00000080:62F2797AC6440D20<1 | VGATHERPF0HINTDPS [ZMM1+RBP+40h],MASK=K2,OPER=7 ; {sint16}. | |ENDPROGRAM t5444`

Expected messages t5444.out
  `I0180 Assembling source file "t5444.htm". I0270 Assembling source "t5444". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5444". "t5444.htm"{64} I0510 Assembling program pass 1. "t5444.htm"{64} I0530 Assembling program pass 2 - final. "t5444.htm"{64} I0660 16bit TINY BIN file "t5444.bin" created, size=136. "t5444.htm"{83} I0650 Program "t5444" assembled in 2 passes with errorlevel 0. "t5444.htm"{83} I0750 Source "t5444" (101 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5444.htm.lst" created, size=1858. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲