| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4146: Machine instructions HINT_NOP in 32bit mode

Tested procedures
  IisHINT_NOP IisHINT_NOPW IisHINT_NOPD IisHINT_NOPQ

Source & expected listing t4146.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,UNDOC=ON | |t4146 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F18C1 | HINT_NOP 0,ECX |00000003:660F18C1 | HINT_NOP 0,CX |00000007:670F1804 | HINT_NOP 0,[SI],DATA=DWORD |0000000B:670F1804 | HINT_NOPD 0,[SI] |0000000F:0F1806 | HINT_NOP 0,[ESI],DATA=DWORD |00000012:0F18C1 | HINT_NOP 00q,ECX |00000015:0F18C9 | HINT_NOP 01q,ECX |00000018:0F18D1 | HINT_NOP 02q,ECX |0000001B:0F18D9 | HINT_NOP 03q,ECX |0000001E:0F18E1 | HINT_NOP 04q,ECX |00000021:0F18E9 | HINT_NOP 05q,ECX |00000024:0F18F1 | HINT_NOP 06q,ECX |00000027:0F18F9 | HINT_NOP 07q,ECX |0000002A:0F19C1 | HINT_NOP 10q,ECX |0000002D:0F19C9 | HINT_NOP 11q,ECX |00000030:0F19D1 | HINT_NOP 12q,ECX |00000033:0F19D9 | HINT_NOP 13q,ECX |00000036:0F19E1 | HINT_NOP 14q,ECX |00000039:0F19E9 | HINT_NOP 15q,ECX |0000003C:0F19F1 | HINT_NOP 16q,ECX |0000003F:0F19F9 | HINT_NOP 17q,ECX |00000042:0F1AC1 | HINT_NOP 20q,ECX |00000045:0F1AC9 | HINT_NOP 21q,ECX |00000048:0F1AD1 | HINT_NOP 22q,ECX |0000004B:0F1AD9 | HINT_NOP 23q,ECX |0000004E:0F1AE1 | HINT_NOP 24q,ECX |00000051:0F1AE9 | HINT_NOP 25q,ECX |00000054:0F1AF1 | HINT_NOP 26q,ECX |00000057:0F1AF9 | HINT_NOP 27q,ECX |0000005A:0F1BC1 | HINT_NOP 30q,ECX |0000005D:0F1BC9 | HINT_NOP 31q,ECX |00000060:0F1BD1 | HINT_NOP 32q,ECX |00000063:0F1BD9 | HINT_NOP 33q,ECX |00000066:0F1BE1 | HINT_NOP 34q,ECX |00000069:0F1BE9 | HINT_NOP 35q,ECX |0000006C:0F1BF1 | HINT_NOP 36q,ECX |0000006F:0F1BF9 | HINT_NOP 37q,ECX |00000072:0F1CC1 | HINT_NOP 40q,ECX |00000075:0F1CC9 | HINT_NOP 41q,ECX |00000078:0F1CD1 | HINT_NOP 42q,ECX |0000007B:0F1CD9 | HINT_NOP 43q,ECX |0000007E:0F1FE1 | HINT_NOP 74q,ECX |00000081:0F1FE9 | HINT_NOP 75q,ECX |00000084:0F1FF1 | HINT_NOP 76q,ECX |00000087:0F1FF9 | HINT_NOP 77q,ECX |0000008A:0F1FF9 | HINT_NOP 63,ECX |0000008D:660F1F3E | HINT_NOPW 63,[ESI] |00000091:670F1F3C | HINT_NOPD 63,[SI] | |ENDPROGRAM t4146`

Expected messages t4146.out
  `I0180 Assembling source file "t4146.htm". I0270 Assembling source "t4146". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4146". "t4146.htm"{58} I0510 Assembling program pass 1. "t4146.htm"{58} I0530 Assembling program pass 2 - final. "t4146.htm"{58} I0660 16bit TINY BIN file "t4146.bin" created, size=149. "t4146.htm"{108} I0650 Program "t4146" assembled in 2 passes with errorlevel 0. "t4146.htm"{108} I0750 Source "t4146" (126 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4146.htm.lst" created, size=2705. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲