| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3665: Machine instructions PF2ID PF2IW PI2FD PI2FW PFCMPEQ PFCMPGE PFCMPGT

Tested procedures
  IidGroup3DNow IidPF2ID IidPF2IW IidPI2FD IidPI2FW IidPFCMPEQ IidPFCMPGE IidPFCMPGT

Source & expected listing t3665.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=28,CPU=X64,MMX=ON,D3NOW=ON,AMD=ON | |t3665 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F0FCE1D | PF2ID MM1,MM6 |0004:0F0FCE1C | PF2IW MM1,MM6 |0008:0F0FCE0D | PI2FD MM1,MM6 |000C:0F0FCE0C | PI2FW MM1,MM6 |0010:0F0FCEB0 | PFCMPEQ MM1,MM6 |0014:0F0FCE90 | PFCMPGE MM1,MM6 |0018:0F0FCEA0 | PFCMPGT MM1,MM6 |001C:0F0F0C1D | PF2ID MM1,[SI] |0020:0F0F0C1C | PF2IW MM1,[SI] |0024:0F0F0C0D | PI2FD MM1,[SI] |0028:0F0F0C0C | PI2FW MM1,[SI] |002C:0F0F0CB0 | PFCMPEQ MM1,[SI] |0030:260F0F0C90 | PFCMPGE MM1,[ES:SI] |0035:670F0F0EA0 | PFCMPGT MM1,[ESI] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F0FCE1D | PF2ID MM1,MM6 |00000004:0F0FCE1C | PF2IW MM1,MM6 |00000008:0F0FCE0D | PI2FD MM1,MM6 |0000000C:0F0FCE0C | PI2FW MM1,MM6 |00000010:0F0FCEB0 | PFCMPEQ MM1,MM6 |00000014:0F0FCE90 | PFCMPGE MM1,MM6 |00000018:0F0FCEA0 | PFCMPGT MM1,MM6 |0000001C:0F0F0E1D | PF2ID MM1,[ESI] |00000020:0F0F0E1C | PF2IW MM1,[ESI] |00000024:0F0F0E0D | PI2FD MM1,[ESI] |00000028:0F0F0E0C | PI2FW MM1,[ESI] |0000002C:0F0F0EB0 | PFCMPEQ MM1,[ESI] |00000030:26670F0F0C90 | PFCMPGE MM1,[ES:SI] |00000036:670F0F0CA0 | PFCMPGT MM1,[SI] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0F0FCE1D | PF2ID MM1,MM6 |00000004:0F0FCE1C | PF2IW MM1,MM6 |00000008:0F0FCE0D | PI2FD MM1,MM6 |0000000C:0F0FCE0C | PI2FW MM1,MM6 |00000010:0F0FCEB0 | PFCMPEQ MM1,MM6 |00000014:0F0FCE90 | PFCMPGE MM1,MM6 |00000018:0F0FCEA0 | PFCMPGT MM1,MM6 |0000001C:0F0F0E1D | PF2ID MM1,[RSI] |00000020:0F0F0E1C | PF2IW MM1,[RSI] |00000024:0F0F0E0D | PI2FD MM1,[RSI] |00000028:0F0F0E0C | PI2FW MM1,[RSI] |0000002C:670F0F0EB0 | PFCMPEQ MM1,[ESI] |00000031:6567420F0F0C1690 | PFCMPGE MM1,[GS:ESI+R10D] |00000039:410F0F08A0 | PFCMPGT MM1,[R8] | |ENDPROGRAM t3665`

Expected messages t3665.out
  `I0180 Assembling source file "t3665.htm". I0270 Assembling source "t3665". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3665". "t3665.htm"{70} I0510 Assembling program pass 1. "t3665.htm"{70} I0530 Assembling program pass 2 - final. "t3665.htm"{70} I0660 16bit TINY BIN file "t3665.bin" created, size=190. "t3665.htm"{116} I0650 Program "t3665" assembled in 2 passes with errorlevel 0. "t3665.htm"{116} I0750 Source "t3665" (134 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3665.htm.lst" created, size=2413. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲