| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5478: Machine instructions VMOVUPS VMOVUPD

Tested procedures
  IizVMOVUPS IizVMOVUPD

Source & expected listing t5478.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5478 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5F810CA | VMOVUPS XMM1,XMM2 |00000004:C5F811D1 | VMOVUPS XMM1,XMM2,CODE=LONG |00000008:62F17C0810CA | VMOVUPS XMM1,XMM2,PREFIX=EVEX |0000000E:62F17C0811D1 | VMOVUPS XMM1,XMM2,CODE=LONG,PREFIX=EVEX |00000014:62F17C8B10CA | VMOVUPS XMM1,XMM2,MASK=K3,ZEROING=ON |0000001A:62F17C0B11D1 | VMOVUPS XMM1,XMM2,MASK=K3,CODE=LONG |00000020:C5FC10CA | VMOVUPS YMM1,YMM2 |00000024:C5FC11D1 | VMOVUPS YMM1,YMM2,CODE=LONG |00000028:62F17C2B10CA | VMOVUPS YMM1,YMM2,MASK=K3 |0000002E:62F17C2B11D1 | VMOVUPS YMM1,YMM2,MASK=K3,CODE=LONG |00000034:62F17C4810CA | VMOVUPS ZMM1,ZMM2 |0000003A:62F17C4811D1 | VMOVUPS ZMM1,ZMM2,CODE=LONG |00000040:62F17C4B10CA | VMOVUPS ZMM1,ZMM2,MASK=K3 |00000046:62F17C4B11D1 | VMOVUPS ZMM1,ZMM2,MASK=K3,CODE=LONG |0000004C:C5F8104D40 | VMOVUPS XMM1,[RBP+40h] |00000051:62F17C0B104D04<4 | VMOVUPS XMM1,[RBP+40h],MASK=K3 |00000058:C5F8115540 | VMOVUPS [RBP+40h],XMM2 |0000005D:62F17C0B115504<4 | VMOVUPS [RBP+40h],XMM2,MASK=K3 |00000064:C5FC104D40 | VMOVUPS YMM1,[RBP+40h] |00000069:62F17C2B104D02<5 | VMOVUPS YMM1,[RBP+40h],MASK=K3 |00000070:C5FC115540 | VMOVUPS [RBP+40h],YMM2 |00000075:62F17C2B115502<5 | VMOVUPS [RBP+40h],YMM2,MASK=K3 |0000007C:62F17C48104D01<6 | VMOVUPS ZMM1,[RBP+40h] |00000083:62F17C4B104D01<6 | VMOVUPS ZMM1,[RBP+40h],MASK=K3 |0000008A:62F17C48115501<6 | VMOVUPS [RBP+40h],ZMM2 |00000091:62F17CCB115501<6 | VMOVUPS [RBP+40h],ZMM2,MASK=K3,ZEROING=ON |00000098: | |00000098:C5F910CA | VMOVUPD XMM1,XMM2 |0000009C:C5F911D1 | VMOVUPD XMM1,XMM2,CODE=LONG |000000A0:62F1FD0810CA | VMOVUPD XMM1,XMM2,PREFIX=EVEX |000000A6:62F1FD0811D1 | VMOVUPD XMM1,XMM2,CODE=LONG,PREFIX=EVEX |000000AC:62F1FD8B10CA | VMOVUPD XMM1,XMM2,MASK=K3,ZEROING=ON |000000B2:62F1FD0B11D1 | VMOVUPD XMM1,XMM2,MASK=K3,CODE=LONG |000000B8:C5FD10CA | VMOVUPD YMM1,YMM2 |000000BC:C5FD11D1 | VMOVUPD YMM1,YMM2,CODE=LONG |000000C0:62F1FD2B10CA | VMOVUPD YMM1,YMM2,MASK=K3 |000000C6:62F1FD2B11D1 | VMOVUPD YMM1,YMM2,MASK=K3,CODE=LONG |000000CC:62F1FD4810CA | VMOVUPD ZMM1,ZMM2 |000000D2:62F1FD4811D1 | VMOVUPD ZMM1,ZMM2,CODE=LONG |000000D8:62F1FD4B10CA | VMOVUPD ZMM1,ZMM2,MASK=K3 |000000DE:62F1FD4B11D1 | VMOVUPD ZMM1,ZMM2,MASK=K3,CODE=LONG |000000E4:C5F9104D40 | VMOVUPD XMM1,[RBP+40h] |000000E9:62F1FD0B104D04<4 | VMOVUPD XMM1,[RBP+40h],MASK=K3 |000000F0:C5F9115540 | VMOVUPD [RBP+40h],XMM2 |000000F5:62F1FD0B115504<4 | VMOVUPD [RBP+40h],XMM2,MASK=K3 |000000FC:C5FD104D40 | VMOVUPD YMM1,[RBP+40h] |00000101:62F1FD2B104D02<5 | VMOVUPD YMM1,[RBP+40h],MASK=K3 |00000108:C5FD115540 | VMOVUPD [RBP+40h],YMM2 |0000010D:62F1FD2B115502<5 | VMOVUPD [RBP+40h],YMM2,MASK=K3 |00000114:62F1FD48104D01<6 | VMOVUPD ZMM1,[RBP+40h] |0000011B:62F1FD4B104D01<6 | VMOVUPD ZMM1,[RBP+40h],MASK=K3 |00000122:62F1FD48115501<6 | VMOVUPD [RBP+40h],ZMM2 |00000129:62F1FDCB115501<6 | VMOVUPD [RBP+40h],ZMM2,MASK=K3,ZEROING=ON | |ENDPROGRAM t5478`

Expected messages t5478.out
  `I0180 Assembling source file "t5478.htm". I0270 Assembling source "t5478". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5478". "t5478.htm"{52} I0510 Assembling program pass 1. "t5478.htm"{52} I0530 Assembling program pass 2 - final. "t5478.htm"{52} I0660 16bit TINY BIN file "t5478.bin" created, size=304. "t5478.htm"{107} I0650 Program "t5478" assembled in 2 passes with errorlevel 0. "t5478.htm"{107} I0750 Source "t5478" (125 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5478.htm.lst" created, size=3484. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲