| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5630: Machine instructions VPRORD VPRORQ VPROLD VPROLQ

Tested procedures
  IiyVPRORD IiyVPRORQ IiyVPROLD IiyVPROLQ

Source & expected listing t5630.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON | |t5630 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F1758C72C203 | VPRORD XMM1,XMM2,3,MASK=K4,ZEROING=ON |00000007:62F175AC72C203 | VPRORD YMM1,YMM2,3,MASK=K4,ZEROING=ON |0000000E:62F175CC72C203 | VPRORD ZMM1,ZMM2,3,MASK=K4,ZEROING=ON |00000015:62F1758C724504<403 | VPRORD XMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |0000001D:62F175AC724502<503 | VPRORD YMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |00000025:62F175CC724501<603 | VPRORD ZMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |0000002D:62F1759C724510<203 | VPRORD XMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |00000035:62F175BC724510<203 | VPRORD YMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |0000003D:62F175DC724510<203 | VPRORD ZMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |00000045:62F1F58C72C203 | VPRORQ XMM1,XMM2,3,MASK=K4,ZEROING=ON |0000004C:62F1F5AC72C203 | VPRORQ YMM1,YMM2,3,MASK=K4,ZEROING=ON |00000053:62F1F5CC72C203 | VPRORQ ZMM1,ZMM2,3,MASK=K4,ZEROING=ON |0000005A:62F1F58C724504<403 | VPRORQ XMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |00000062:62F1F5AC724502<503 | VPRORQ YMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |0000006A:62F1F5CC724501<603 | VPRORQ ZMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |00000072:62F1F59C724508<303 | VPRORQ XMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |0000007A:62F1F5BC724508<303 | VPRORQ YMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |00000082:62F1F5DC724508<303 | VPRORQ ZMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |0000008A:62F1758C72CA03 | VPROLD XMM1,XMM2,3,MASK=K4,ZEROING=ON |00000091:62F175AC72CA03 | VPROLD YMM1,YMM2,3,MASK=K4,ZEROING=ON |00000098:62F175CC72CA03 | VPROLD ZMM1,ZMM2,3,MASK=K4,ZEROING=ON |0000009F:62F1758C724D04<403 | VPROLD XMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |000000A7:62F175AC724D02<503 | VPROLD YMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |000000AF:62F175CC724D01<603 | VPROLD ZMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |000000B7:62F1759C724D10<203 | VPROLD XMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |000000BF:62F175BC724D10<203 | VPROLD YMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |000000C7:62F175DC724D10<203 | VPROLD ZMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |000000CF:62F1F58C72CA03 | VPROLQ XMM1,XMM2,3,MASK=K4,ZEROING=ON |000000D6:62F1F5AC72CA03 | VPROLQ YMM1,YMM2,3,MASK=K4,ZEROING=ON |000000DD:62F1F5CC72CA03 | VPROLQ ZMM1,ZMM2,3,MASK=K4,ZEROING=ON |000000E4:62F1F58C724D04<403 | VPROLQ XMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |000000EC:62F1F5AC724D02<503 | VPROLQ YMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |000000F4:62F1F5CC724D01<603 | VPROLQ ZMM1,[RBP+40h],3,MASK=K4,ZEROING=ON |000000FC:62F1F59C724D08<303 | VPROLQ XMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |00000104:62F1F5BC724D08<303 | VPROLQ YMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON |0000010C:62F1F5DC724D08<303 | VPROLQ ZMM1,[RBP+40h],3,MASK=K4,ZEROING=ON,BCST=ON | |ENDPROGRAM t5630`

Expected messages t5630.out
  `I0180 Assembling source file "t5630.htm". I0270 Assembling source "t5630". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5630". "t5630.htm"{58} I0510 Assembling program pass 1. "t5630.htm"{58} I0530 Assembling program pass 2 - final. "t5630.htm"{58} I0660 16bit TINY BIN file "t5630.bin" created, size=276. "t5630.htm"{96} I0650 Program "t5630" assembled in 2 passes with errorlevel 0. "t5630.htm"{96} I0750 Source "t5630" (114 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5630.htm.lst" created, size=3037. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲