| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4600: Machine instructions VAESENC VAESENCLAST VAESDEC VAESDECLAST VAESIMC VAESKEYGENASSIST

Tested procedures
  IiaVAESENC IiaVAESENCLAST IiaVAESDEC IiaVAESDECLAST IiaVAESIMC IiaVAESKEYGENASSIST

Source & expected listing t4600.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,SIMD=AVX,AES=ON | |t4600 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E269DCCB | VAESENC XMM1,XMM2,XMM3 |00000005:C4E269DDCB | VAESENCLAST XMM1,XMM2,XMM3 |0000000A:C4E269DECB | VAESDEC XMM1,XMM2,XMM3 |0000000F:C4E269DFCB | VAESDECLAST XMM1,XMM2,XMM3 |00000014:C4E279DBCA | VAESIMC XMM1,XMM2 |00000019:C4E379DFCA03 | VAESKEYGENASSIST XMM1,XMM2,3 |0000001F:C4E269DC0E | VAESENC XMM1,XMM2,[RSI] |00000024:C4E269DD0E | VAESENCLAST XMM1,XMM2,[RSI] |00000029:C4E269DE0E | VAESDEC XMM1,XMM2,[RSI] |0000002E:C4E269DF0E | VAESDECLAST XMM1,XMM2,[RSI] |00000033:C4E279DB0E | VAESIMC XMM1,[RSI] |00000038:C4E379DF0E03 | VAESKEYGENASSIST XMM1,[RSI],3 | |ENDPROGRAM t4600`

Expected messages t4600.out
  `I0180 Assembling source file "t4600.htm". I0270 Assembling source "t4600". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4600". "t4600.htm"{64} I0510 Assembling program pass 1. "t4600.htm"{64} I0530 Assembling program pass 2 - final. "t4600.htm"{64} I0660 16bit TINY BIN file "t4600.bin" created, size=62. "t4600.htm"{78} I0650 Program "t4600" assembled in 2 passes with errorlevel 0. "t4600.htm"{78} I0750 Source "t4600" (96 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4600.htm.lst" created, size=910. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲