| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6245: Machine instructions POPCNT LZCNT TZCNT TZCNTI in 32bit mode

Tested procedures
  IigPOPCNT IigLZCNT IigTZCNT IiyTZCNTI

Source & expected listing t6245.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,MVEX=ON,ABM=ON,SPEC=ON | |t6245 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:F30FB80E | POPCNT ECX,[ESI] |00000004:F30FB8CA | POPCNT ECX,EDX |00000008:C5FAB8CA | POPCNT ECX,EDX,PREFIX=VEX |0000000C:C4E17AB8CA | POPCNT ECX,EDX,PREFIX=VEX3 |00000011:F30FBD0E | LZCNT ECX,[ESI] |00000015:F30FBDCA | LZCNT ECX,EDX |00000019:C5FABDCA | LZCNT ECX,EDX,PREFIX=VEX |0000001D:C4E17ABDCA | LZCNT ECX,EDX,PREFIX=VEX3 |00000022:F30FBC0E | TZCNT ECX,[ESI] |00000026:F30FBCCA | TZCNT ECX,EDX |0000002A:C5FABCCA | TZCNT ECX,EDX,PREFIX=VEX |0000002E:C4E17ABCCA | TZCNT ECX,EDX,PREFIX=VEX3 |00000033:C5FBBCCA | TZCNTI ECX,EDX |00000037:C4E17BBCCA | TZCNTI ECX,EDX,PREFIX=VEX3 | |ENDPROGRAM t6245`

Expected messages t6245.out
  `I0180 Assembling source file "t6245.htm". I0270 Assembling source "t6245". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6245". "t6245.htm"{58} I0510 Assembling program pass 1. "t6245.htm"{58} I0530 Assembling program pass 2 - final. "t6245.htm"{58} I0660 16bit TINY BIN file "t6245.bin" created, size=60. "t6245.htm"{74} I0650 Program "t6245" assembled in 2 passes with errorlevel 0. "t6245.htm"{74} I0750 Source "t6245" (92 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6245.htm.lst" created, size=1061. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲