| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3335: Machine instructions BTR BTRW BTRD BTRQ

Tested procedures
  IigBTR IigBTRW IigBTRD IigBTRQ

Source & expected listing t3335.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,CPU=X64 | |t3335 PROGRAM FORMAT=BIN,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0FB3D1 | BTR CX,DX |0003:660FB3D1 | BTR ECX,EDX |0007:0FB314 | BTR [SI],DX |000A:660FB314 | BTR [SI],EDX |000E:0FB316[7C00] | BTR [MemWord],DX |0013:660FB316[7800] | BTR [MemDword],EDX |0019:0FBAF102 | BTR CX,2 |001D:660FBAF102 | BTR ECX,2 |0022:0FBA36[7C00]02 | BTR [MemWord],2 |0028:660FBA36[7800]02 | BTR [MemDword],2 |002F:0FBA3402 | BTRW [SI],2 |0033:660FBA3402 | BTRD [SI],2 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660FB3D1 | BTR CX,DX |00000004:0FB3D1 | BTR ECX,EDX |00000007:660FB316 | BTR [ESI],DX |0000000B:0FB316 | BTR [ESI],EDX |0000000E:660FB315[7C000000] | BTR [MemWord],DX |00000016:0FB315[78000000] | BTR [MemDword],EDX |0000001D:660FBAF102 | BTR CX,2 |00000022:0FBAF102 | BTR ECX,2 |00000026:660FBA35[7C000000]02 | BTR [MemWord],2 |0000002F:0FBA35[78000000]02 | BTR [MemDword],2 |00000037:660FBA3602 | BTRW [ESI],2 |0000003C:0FBA3602 | BTRD [ESI],2 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:660FB3D1 | BTR CX,DX |00000004:0FB3D1 | BTR ECX,EDX |00000007:480FB3D1 | BTR RCX,RDX |0000000B:4D0FB3D1 | BTR R9,R10 |0000000F:660FB316 | BTR [RSI],DX |00000013:0FB316 | BTR [RSI],EDX |00000016:480FB316 | BTR [RSI],RDX |0000001A:660FB3155A000000 | BTR [MemWord],DX |00000022:0FB3154F000000 | BTR [MemDword],EDX |00000029:480FB3153F000000 | BTR [MemQword],RDX |00000031:660FBAF102 | BTR CX,2 |00000036:0FBAF102 | BTR ECX,2 |0000003A:480FBAF102 | BTR RCX,2 |0000003F:490FBAF102 | BTR R9,2 |00000044:660FBA352F00000002 | BTR [MemWord],2 |0000004D:0FBA352300000002 | BTR [MemDword],2 |00000055:480FBA351200000002 | BTR [MemQword],2 |0000005E:660FBA3602 | BTRW [RSI],2 |00000063:0FBA3602 | BTRD [RSI],2 |00000067:480FBA3602 | BTRQ [RSI],2 |0000006C:0F1F4000 | ALIGN QWORD |00000070:0000000000000000 |MemQword DQ Q |00000078:00000000 |MemDword DD D |0000007C:0000 |MemWord DW W | |ENDPROGRAM t3335`

Expected messages t3335.out
  `I0180 Assembling source file "t3335.htm". I0270 Assembling source "t3335". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3335". "t3335.htm"{58} I0510 Assembling program pass 1. "t3335.htm"{58} I0510 Assembling program pass 2. "t3335.htm"{58} I0510 Assembling program pass 3. "t3335.htm"{58} I0530 Assembling program pass 4 - final. "t3335.htm"{58} I0660 16bit TINY BIN file "t3335.bin" created, size=254. "t3335.htm"{110} I0650 Program "t3335" assembled in 4 passes with errorlevel 0. "t3335.htm"{110} I0750 Source "t3335" (130 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3335.htm.lst" created, size=2812. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲