| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6226: Machine instruction KMOV

Tested procedures
  IikKMOV

Source & expected listing t6226.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,SIMD=AVX512,MVEX=ENABLE | |t6226 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5F890CA | KMOV K1,K2 |00000004:C5F892CA | KMOV K1,EDX |00000008:C5F893CA | KMOV ECX,K2 |0000000C:C4E17890CA | KMOV K1,K2,PREFIX=VEX3 |00000011:C4E17892CA | KMOV K1,EDX,PREFIX=VEX3 |00000016:C4E17893CA | KMOV ECX,K2,PREFIX=VEX3 | |ENDPROGRAM t6226`

Expected messages t6226.out
  `I0180 Assembling source file "t6226.htm". I0270 Assembling source "t6226". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6226". "t6226.htm"{49} I0510 Assembling program pass 1. "t6226.htm"{49} I0530 Assembling program pass 2 - final. "t6226.htm"{49} I0660 16bit TINY BIN file "t6226.bin" created, size=27. "t6226.htm"{57} I0650 Program "t6226" assembled in 2 passes with errorlevel 0. "t6226.htm"{57} I0750 Source "t6226" (75 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6226.htm.lst" created, size=543. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲