| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3520: Machine instructions FPREM FYL2XP1 FSQRT FSINCOS FRNDINT FSCALE FSIN FCOS

Tested procedures
  IifFPREM IifFYL2XP1 IifFSQRT IifFSINCOS IifFRNDINT IifFSCALE IifFSIN IifFCOS

Source & expected listing t3520.htm.lst
  `| |EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=24, CPU=386, FPU=ON | |t3520 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:D9F8 | FPREM |00000002:D9F8 | FPREM ST0 |00000004:D9F9 | FYL2XP1 |00000006:D9F9 | FYL2XP1 ST0 |00000008:D9FA | FSQRT |0000000A:D9FA | FSQRT ST0 |0000000C:D9FB | FSINCOS |0000000E:D9FB | FSINCOS ST0 |00000010:D9FC | FRNDINT |00000012:D9FC | FRNDINT ST0 |00000014:D9FD | FSCALE |00000016:D9FD | FSCALE ST0 |00000018:D9FE | FSIN |0000001A:D9FE | FSIN ST0 |0000001C:D9FF | FCOS |0000001E:D9FF | FCOS ST0 | |ENDPROGRAM t3520`

Expected messages t3520.out
  `I0180 Assembling source file "t3520.htm". I0270 Assembling source "t3520". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3520". "t3520.htm"{70} I0510 Assembling program pass 1. "t3520.htm"{70} I0530 Assembling program pass 2 - final. "t3520.htm"{70} I0660 16bit TINY BIN file "t3520.bin" created, size=32. "t3520.htm"{88} I0650 Program "t3520" assembled in 2 passes with errorlevel 0. "t3520.htm"{88} I0750 Source "t3520" (106 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3520.htm.lst" created, size=822. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲