| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3680: Machine instructions PFRCP PFRCPV PFRSQRT PFRSQRTV PFMUL PMULHRW PMULHRWA

Tested procedures
  IidGroup3DNow IidPFRCP IidPFRCPV IidPFRSQRT IidPFRSQRTV IidPFMUL IidPMULHRW IidPMULHRWA

Source & expected listing t3680.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=28,CPU=X64,MMX=ON,D3NOW=ON,CYRIX=ON,AMD=ON | |t3680 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F0FCE96 | PFRCP MM1,MM6 |0004:0F0FCE86 | PFRCPV MM1,MM6 |0008:0F0FCE97 | PFRSQRT MM1,MM6 |000C:0F0FCE87 | PFRSQRTV MM1,MM6 |0010:0F0FCEB4 | PFMUL MM1,MM6 |0014:0F0FCEB7 | PMULHRW MM1,MM6 |0018:0F0FCEB7 | PMULHRWA MM1,MM6 |001C:0F0F0C96 | PFRCP MM1,[SI] |0020:0F0F0C86 | PFRCPV MM1,[SI] |0024:0F0F0C97 | PFRSQRT MM1,[SI] |0028:0F0F0C87 | PFRSQRTV MM1,[SI] |002C:0F0F0CB4 | PFMUL MM1,[SI] |0030:260F0F0CB7 | PMULHRW MM1,[ES:SI] |0035:670F0F0EB7 | PMULHRWA MM1,[ESI] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F0FCE96 | PFRCP MM1,MM6 |00000004:0F0FCE86 | PFRCPV MM1,MM6 |00000008:0F0FCE97 | PFRSQRT MM1,MM6 |0000000C:0F0FCE87 | PFRSQRTV MM1,MM6 |00000010:0F0FCEB4 | PFMUL MM1,MM6 |00000014:0F0FCEB7 | PMULHRW MM1,MM6 |00000018:0F0FCEB7 | PMULHRWA MM1,MM6 |0000001C:0F0F0E96 | PFRCP MM1,[ESI] |00000020:0F0F0E86 | PFRCPV MM1,[ESI] |00000024:0F0F0E97 | PFRSQRT MM1,[ESI] |00000028:0F0F0E87 | PFRSQRTV MM1,[ESI] |0000002C:0F0F0EB4 | PFMUL MM1,[ESI] |00000030:26670F0F0CB7 | PMULHRW MM1,[ES:SI] |00000036:670F0F0CB7 | PMULHRWA MM1,[SI] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0F0FCE96 | PFRCP MM1,MM6 |00000004:0F0FCE86 | PFRCPV MM1,MM6 |00000008:0F0FCE97 | PFRSQRT MM1,MM6 |0000000C:0F0FCE87 | PFRSQRTV MM1,MM6 |00000010:0F0FCEB4 | PFMUL MM1,MM6 |00000014:0F0FCEB7 | PMULHRW MM1,MM6 |00000018:0F0FCEB7 | PMULHRWA MM1,MM6 |0000001C:0F0F0E96 | PFRCP MM1,[RSI] |00000020:0F0F0E86 | PFRCPV MM1,[RSI] |00000024:0F0F0E97 | PFRSQRT MM1,[RSI] |00000028:0F0F0E87 | PFRSQRTV MM1,[RSI] |0000002C:0F0F0EB4 | PFMUL MM1,[RSI] |00000030:6567420F0F0C16B7 | PMULHRW MM1,[GS:ESI+R10D] |00000038:410F0F08B7 | PMULHRWA MM1,[R8] | |ENDPROGRAM t3680`

Expected messages t3680.out
  `I0180 Assembling source file "t3680.htm". I0270 Assembling source "t3680". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3680". "t3680.htm"{70} I0510 Assembling program pass 1. "t3680.htm"{70} I0530 Assembling program pass 2 - final. "t3680.htm"{70} I0660 16bit TINY BIN file "t3680.bin" created, size=189. "t3680.htm"{116} I0650 Program "t3680" assembled in 2 passes with errorlevel 0. "t3680.htm"{116} I0750 Source "t3680" (134 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3680.htm.lst" created, size=2464. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲