| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5404: Machine instructions VFMADD132SD VFMADD213SD VFMADD231SD VFMSUB132SD VFMSUB213SD VFMSUB231SD

Tested procedures
  IibVFMADD132SD IibVFMADD213SD IibVFMADD231SD IibVFMSUB132SD IibVFMSUB213SD IibVFMSUB231SD

Source & expected listing t5404.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,DUMPALL=OFF,CPU=X64,SIMD=AVX512,FMA=ON,EVEX=ON | |t5404 PROGRAM FORMAT=BIN,MODEL=TINY,WIDTH=16,LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E2E999CB | VFMADD132SD XMM1,XMM2,XMM3 |00000005:62F2ED5899CB | VFMADD132SD XMM1,XMM2,XMM3,ROUND=UP |0000000B:62F2ED8C99CB | VFMADD132SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000011:62F2ED8C994D08<3 | VFMADD132SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000018:C4E2E9A9CB | VFMADD213SD XMM1,XMM2,XMM3 |0000001D:62F2ED58A9CB | VFMADD213SD XMM1,XMM2,XMM3,ROUND=UP |00000023:62F2ED8CA9CB | VFMADD213SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000029:62F2ED8CA94D08<3 | VFMADD213SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000030:C4E2E9B9CB | VFMADD231SD XMM1,XMM2,XMM3 |00000035:62F2ED58B9CB | VFMADD231SD XMM1,XMM2,XMM3,ROUND=UP |0000003B:62F2ED8CB9CB | VFMADD231SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000041:62F2ED8CB94D08<3 | VFMADD231SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000048:C4E2E99BCB | VFMSUB132SD XMM1,XMM2,XMM3 |0000004D:62F2ED589BCB | VFMSUB132SD XMM1,XMM2,XMM3,ROUND=UP |00000053:62F2ED8C9BCB | VFMSUB132SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000059:62F2ED8C9B4D08<3 | VFMSUB132SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000060:C4E2E9ABCB | VFMSUB213SD XMM1,XMM2,XMM3 |00000065:62F2ED58ABCB | VFMSUB213SD XMM1,XMM2,XMM3,ROUND=UP |0000006B:62F2ED8CABCB | VFMSUB213SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000071:62F2ED8CAB4D08<3 | VFMSUB213SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000078:C4E2E9BBCB | VFMSUB231SD XMM1,XMM2,XMM3 |0000007D:62F2ED58BBCB | VFMSUB231SD XMM1,XMM2,XMM3,ROUND=UP |00000083:62F2ED8CBBCB | VFMSUB231SD XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000089:62F2ED8CBB4D08<3 | VFMSUB231SD XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON | |ENDPROGRAM t5404`

Expected messages t5404.out
  `I0180 Assembling source file "t5404.htm". I0270 Assembling source "t5404". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5404". "t5404.htm"{64} I0510 Assembling program pass 1. "t5404.htm"{64} I0530 Assembling program pass 2 - final. "t5404.htm"{64} I0660 16bit TINY BIN file "t5404.bin" created, size=144. "t5404.htm"{90} I0650 Program "t5404" assembled in 2 passes with errorlevel 0. "t5404.htm"{90} I0750 Source "t5404" (108 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5404.htm.lst" created, size=2179. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲