| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4310: Machine instructions BNDCL BNDCU BNDCN BNDMK

Tested procedures
  IisBNDCL IisBNDCU IisBNDCN IisBNDMK

Source & expected listing t4310.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,DUMPALL=OFF,CPU=X64,MPX=ENABLED | |t4310 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:F30F1A0E | BNDCL BND1,[ESI] |00000004:F30F1ACE | BNDCL BND1,ESI |00000008:F20F1A0E | BNDCU BND1,[ESI] |0000000C:F20F1ACE | BNDCU BND1,ESI |00000010:F20F1B0E | BNDCN BND1,[ESI] |00000014:F20F1BCE | BNDCN BND1,ESI |00000018:F30F1B0E | BNDMK BND1,[ESI] |0000001C:F30F1B0C96 | BNDMK BND1,[ESI+4*EDX] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:F30F1A0E | BNDCL BND1,[RSI] |00000004:67F30F1A0E | BNDCL BND1,[ESI] |00000009:F30F1ACE | BNDCL BND1,RSI |0000000D:F30F1ACE | BNDCL BND1,ESI |00000011:F20F1A0E | BNDCU BND1,[RSI] |00000015:67F20F1A0E | BNDCU BND1,[ESI] |0000001A:F20F1ACE | BNDCU BND1,RSI |0000001E:F20F1ACE | BNDCU BND1,ESI |00000022:F20F1B0E | BNDCN BND1,[RSI] |00000026:67F20F1B0E | BNDCN BND1,[ESI] |0000002B:F20F1BCE | BNDCN BND1,RSI |0000002F:F20F1BCE | BNDCN BND1,ESI |00000033:F30F1B0E | BNDMK BND1,[RSI] |00000037:67F30F1B0E | BNDMK BND1,[ESI] |0000003C:F3420F1B0CA6 | BNDMK BND1,[RSI+4*R12] | |ENDPROGRAM t4310`

Expected messages t4310.out
  `I0180 Assembling source file "t4310.htm". I0270 Assembling source "t4310". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4310". "t4310.htm"{58} I0510 Assembling program pass 1. "t4310.htm"{58} I0530 Assembling program pass 2 - final. "t4310.htm"{58} I0660 16bit TINY BIN file "t4310.bin" created, size=114. "t4310.htm"{84} I0650 Program "t4310" assembled in 2 passes with errorlevel 0. "t4310.htm"{84} I0750 Source "t4310" (102 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4310.htm.lst" created, size=1608. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲