| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3421: Machine instructions LMSW SMSW CL1INVMB ALTINST

Tested procedures
  IisLMSW IisSMSW IisCL1INVMB IisALTINST

Source & expected listing t3421.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=35, CPU=X64, PRIV=ON | |t3421 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0F01F1 | LMSW CX |0003:0F01F1 | LMSW ECX |0006:0F0134 | LMSW [SI] |0009:670F0136 | LMSW [ESI] |000D:0F01E1 | SMSW CX |0010:660F01E1 | SMSW ECX |0014:0F0124 | SMSW [SI] |0017:670F0126 | SMSW [ESI] | | EUROASM SPEC=ON |001B:0F0A | CL1INVMB | | EUROASM VIA=ON |001D:0F3F | ALTINST |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F01F1 | LMSW CX |00000003:0F01F1 | LMSW ECX |00000006:670F0134 | LMSW [SI] |0000000A:0F0136 | LMSW [ESI] |0000000D:660F01E1 | SMSW CX |00000011:0F01E1 | SMSW ECX |00000014:670F0124 | SMSW [SI] |00000018:0F0126 | SMSW [ESI] |0000001B:0F0A | CL1INVMB |0000001D:0F3F | ALTINST |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0F01F1 | LMSW CX |00000003:0F01F1 | LMSW ECX |00000006:0F01F1 | LMSW RCX |00000009:410F01F1 | LMSW R9D |0000000D:0F0136 | LMSW [RSI] |00000010:670F0136 | LMSW [ESI] |00000014:660F01E1 | SMSW CX |00000018:0F01E1 | SMSW ECX |0000001B:480F01E1 | SMSW RCX |0000001F:0F0126 | SMSW [RSI] |00000022:670F0126 | SMSW [ESI] |00000026:0F0A | CL1INVMB |00000028:0F3F | ALTINST | |ENDPROGRAM t3421`

Expected messages t3421.out
  `I0180 Assembling source file "t3421.htm". I0270 Assembling source "t3421". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3421". "t3421.htm"{58} I0510 Assembling program pass 1. "t3421.htm"{58} I0530 Assembling program pass 2 - final. "t3421.htm"{58} I0660 16bit TINY BIN file "t3421.bin" created, size=106. "t3421.htm"{97} I0650 Program "t3421" assembled in 2 passes with errorlevel 0. "t3421.htm"{97} I0750 Source "t3421" (115 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3421.htm.lst" created, size=2097. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲