| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5258: Machine instructions VBLENDVPS VBLENDVPD VPBLENDVB

Tested procedures
  IiyVBLENDVPS IiyVBLENDVPD IiyVPBLENDVB

Source & expected listing t5258.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX | |t5258 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E3694ACB40 | VBLENDVPS XMM1,XMM2,XMM3,XMM4 |00000006:C4E36D4ACB40 | VBLENDVPS YMM1,YMM2,YMM3,YMM4 |0000000C:C4E3694A0E40 | VBLENDVPS XMM1,XMM2,[RSI],XMM4 |00000012:C4E36D4A0E40 | VBLENDVPS YMM1,YMM2,[RSI],YMM4 |00000018:C4E3694BCB40 | VBLENDVPD XMM1,XMM2,XMM3,XMM4 |0000001E:C4E36D4BCB40 | VBLENDVPD YMM1,YMM2,YMM3,YMM4 |00000024:C4E3694B0E40 | VBLENDVPD XMM1,XMM2,[RSI],XMM4 |0000002A:C4E36D4B0E40 | VBLENDVPD YMM1,YMM2,[RSI],YMM4 |00000030:C4E3694CCB40 | VPBLENDVB XMM1,XMM2,XMM3,XMM4 |00000036:C4E36D4CCB40 | VPBLENDVB YMM1,YMM2,YMM3,YMM4 |0000003C:C4E3694C0E40 | VPBLENDVB XMM1,XMM2,[RSI],XMM4 |00000042:C4E36D4C0E40 | VPBLENDVB YMM1,YMM2,[RSI],YMM4 |00000048:C4432D4CCBC0 | VPBLENDVB YMM9,YMM10,YMM11,YMM12 | |ENDPROGRAM t5258`

Expected messages t5258.out
  `I0180 Assembling source file "t5258.htm". I0270 Assembling source "t5258". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5258". "t5258.htm"{55} I0510 Assembling program pass 1. "t5258.htm"{55} I0530 Assembling program pass 2 - final. "t5258.htm"{55} I0660 16bit TINY BIN file "t5258.bin" created, size=78. "t5258.htm"{70} I0650 Program "t5258" assembled in 2 passes with errorlevel 0. "t5258.htm"{70} I0750 Source "t5258" (88 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5258.htm.lst" created, size=1104. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲