| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3436: Machine instructions CLFLUSH CLFLUSHOPT CLZERO SWAPGS

Tested procedures
  IisCLFLUSH IisCLFLUSHOPT IisCLZERO IisSWAPGS

Source & expected listing t3436.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,SIMD=SSE2 | |t3436 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0FAE3C | CLFLUSH [SI] |0003:670FAE3E | CLFLUSH [ESI] |0007:660FAE3D | CLFLUSHOPT [DI] |000B:66670FAE3F | CLFLUSHOPT [EDI] | | EUROASM AMD=ENABLED |0010:0F01FC | CLZERO |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0FAE3E | CLFLUSH [ESI] |00000003:670FAE3C | CLFLUSH [SI] |00000007:660FAE3F | CLFLUSHOPT [EDI] |0000000B:66670FAE3D | CLFLUSHOPT [DI] |00000010:0F01FC | CLZERO |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0FAE3E | CLFLUSH [RSI] |00000003:670FAE3E | CLFLUSH [ESI] |00000007:410FAE7C2C10 | CLFLUSH [R12+RBP+16] |0000000D:660FAE3F | CLFLUSHOPT [RDI] |00000011:66670FAE3F | CLFLUSHOPT [EDI] |00000016:0F01FC | CLZERO | | EUROASM PRIV=ENABLED |00000019:0F01F8 | SWAPGS | |ENDPROGRAM t3436`

Expected messages t3436.out
  `I0180 Assembling source file "t3436.htm". I0270 Assembling source "t3436". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3436". "t3436.htm"{58} I0510 Assembling program pass 1. "t3436.htm"{58} I0530 Assembling program pass 2 - final. "t3436.htm"{58} I0660 16bit TINY BIN file "t3436.bin" created, size=92. "t3436.htm"{81} I0650 Program "t3436" assembled in 2 passes with errorlevel 0. "t3436.htm"{81} I0750 Source "t3436" (99 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3436.htm.lst" created, size=1162. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲