| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4510: Machine instructions BLCFILL BLSFILL BLCS TZMSK BLCIC BLSIC T1MSKC

Tested procedures
  IixBLCFILL IixBLSFILL IixBLCS IixTZMSK IixBLCIC IixBLSIC IixT1MSKC

Source & expected listing t4510.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=28,CPU=X64,SIMD=AVX,AMD=ENABLED,XOP=ENABLED | |t4510 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:8FE97001CA | BLCFILL ECX,EDX |00000005:8FE9F001CA | BLCFILL RCX,RDX |0000000A:8FE970010E | BLCFILL ECX,[RSI] |0000000F:8FE9F0010E | BLCFILL RCX,[RSI] |00000014:8FE97001D2 | BLSFILL ECX,EDX |00000019:8FE9F001D2 | BLSFILL RCX,RDX |0000001E:8FE9700116 | BLSFILL ECX,[RSI] |00000023:8FE9F00116 | BLSFILL RCX,[RSI] |00000028:8FE97001DA | BLCS ECX,EDX |0000002D:8FE9F001DA | BLCS RCX,RDX |00000032:8FE970011E | BLCS ECX,[RSI] |00000037:8FE9F0011E | BLCS RCX,[RSI] |0000003C:8FE97001E2 | TZMSK ECX,EDX |00000041:8FE9F001E2 | TZMSK RCX,RDX |00000046:8FE9700126 | TZMSK ECX,[RSI] |0000004B:8FE9F00126 | TZMSK RCX,[RSI] |00000050:8FE97001EA | BLCIC ECX,EDX |00000055:8FE9F001EA | BLCIC RCX,RDX |0000005A:8FE970012E | BLCIC ECX,[RSI] |0000005F:8FE9F0012E | BLCIC RCX,[RSI] |00000064:8FE97001F2 | BLSIC ECX,EDX |00000069:8FE9F001F2 | BLSIC RCX,RDX |0000006E:8FE9700136 | BLSIC ECX,[RSI] |00000073:8FE9F00136 | BLSIC RCX,[RSI] |00000078:8FE97001FA | T1MSKC ECX,EDX |0000007D:8FE9F001FA | T1MSKC RCX,RDX |00000082:8FE970013E | T1MSKC ECX,[RSI] |00000087:8FE9F0013E | T1MSKC RCX,[RSI] | | ENDPROGRAM t4510`

Expected messages t4510.out
  `I0180 Assembling source file "t4510.htm". I0270 Assembling source "t4510". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4510". "t4510.htm"{67} I0510 Assembling program pass 1. "t4510.htm"{67} I0530 Assembling program pass 2 - final. "t4510.htm"{67} I0660 16bit TINY BIN file "t4510.bin" created, size=140. "t4510.htm"{97} I0650 Program "t4510" assembled in 2 passes with errorlevel 0. "t4510.htm"{97} I0750 Source "t4510" (115 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4510.htm.lst" created, size=1625. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲