| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4610: Machine instructions VPCMPESTRM VPCMPESTRI VPCMPISTRM VPCMPISTRI

Tested procedures
  IiaVPCMPESTRM IiaVPCMPESTRI IiaVPCMPISTRM IiaVPCMPISTRI

Source & expected listing t4610.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,SIMD=AVX,AMD=ON | |t4610 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E37960CA03 | VPCMPESTRM XMM1,XMM2,3 |00000006:C4E37960CA03 | VPCMPESTRM XMM1,XMM2,3,DATA=DWORD |0000000C:C4E3F960CA03 | VPCMPESTRM XMM1,XMM2,3,DATA=QWORD |00000012:C4E37961CA03 | VPCMPESTRI XMM1,XMM2,3 |00000018:C4E37961CA03 | VPCMPESTRI XMM1,XMM2,3,DATA=DWORD |0000001E:C4E3F961CA03 | VPCMPESTRI XMM1,XMM2,3,DATA=QWORD |00000024:C4E37962CA03 | VPCMPISTRM XMM1,XMM2,3 |0000002A:C4E37963CA03 | VPCMPISTRI XMM1,XMM2,3 |00000030:C4E379600E03 | VPCMPESTRM XMM1,[RSI],3 |00000036:C4E379610E03 | VPCMPESTRI XMM1,[RSI],3 |0000003C:C4E379620E03 | VPCMPISTRM XMM1,[RSI],3 |00000042:C4E379630E03 | VPCMPISTRI XMM1,[RSI],3 | |ENDPROGRAM t4610`

Expected messages t4610.out
  `I0180 Assembling source file "t4610.htm". I0270 Assembling source "t4610". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4610". "t4610.htm"{58} I0510 Assembling program pass 1. "t4610.htm"{58} I0530 Assembling program pass 2 - final. "t4610.htm"{58} I0660 16bit TINY BIN file "t4610.bin" created, size=72. "t4610.htm"{72} I0650 Program "t4610" assembled in 2 passes with errorlevel 0. "t4610.htm"{72} I0750 Source "t4610" (90 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4610.htm.lst" created, size=910. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲