| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5642: Machine instructions VPMULUDQ VPMADDWD VPSADBW

Tested procedures
  IizVPMULUDQ IizVPMADDWD IizVPSADBW

Source & expected listing t5642.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5642 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5E9F4CB | VPMULUDQ XMM1,XMM2,XMM3 |00000004:C5EDF4CB | VPMULUDQ YMM1,YMM2,YMM3 |00000008:C4E169F4CB | VPMULUDQ XMM1,XMM2,XMM3,PREFIX=VEX3 |0000000D:C4E16DF4CB | VPMULUDQ YMM1,YMM2,YMM3,PREFIX=VEX3 |00000012:62F1ED0CF4CB | VPMULUDQ XMM1,XMM2,XMM3,MASK=K4 |00000018:62F1ED2CF4CB | VPMULUDQ YMM1,YMM2,YMM3,MASK=K4 |0000001E:62F1ED4CF4CB | VPMULUDQ ZMM1,ZMM2,ZMM3,MASK=K4 |00000024:C5E9F44D40 | VPMULUDQ XMM1,XMM2,[RBP+40h] |00000029:C5EDF44D40 | VPMULUDQ YMM1,YMM2,[RBP+40h] |0000002E:C4E169F44D40 | VPMULUDQ XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000034:C4E16DF44D40 | VPMULUDQ YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |0000003A:62F1ED0CF44D04<4 | VPMULUDQ XMM1,XMM2,[RBP+40h],MASK=K4 |00000041:62F1ED2CF44D02<5 | VPMULUDQ YMM1,YMM2,[RBP+40h],MASK=K4 |00000048:62F1ED4CF44D01<6 | VPMULUDQ ZMM1,ZMM2,[RBP+40h],MASK=K4 |0000004F:62F1ED1CF44D08<3 | VPMULUDQ XMM1,XMM2,[RBP+40h],MASK=K4,BCST=ON |00000056:62F1ED3CF44D08<3 | VPMULUDQ YMM1,YMM2,[RBP+40h],MASK=K4,BCST=ON |0000005D:62F1ED5CF44D08<3 | VPMULUDQ ZMM1,ZMM2,[RBP+40h],MASK=K4,BCST=ON |00000064:C5E9F5CB | VPMADDWD XMM1,XMM2,XMM3 |00000068:C5EDF5CB | VPMADDWD YMM1,YMM2,YMM3 |0000006C:C4E169F5CB | VPMADDWD XMM1,XMM2,XMM3,PREFIX=VEX3 |00000071:C4E16DF5CB | VPMADDWD YMM1,YMM2,YMM3,PREFIX=VEX3 |00000076:62F16D0CF5CB | VPMADDWD XMM1,XMM2,XMM3,MASK=K4 |0000007C:62F16D2CF5CB | VPMADDWD YMM1,YMM2,YMM3,MASK=K4 |00000082:62F16D4CF5CB | VPMADDWD ZMM1,ZMM2,ZMM3,MASK=K4 |00000088:C5E9F54D40 | VPMADDWD XMM1,XMM2,[RBP+40h] |0000008D:C5EDF54D40 | VPMADDWD YMM1,YMM2,[RBP+40h] |00000092:C4E169F54D40 | VPMADDWD XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000098:C4E16DF54D40 | VPMADDWD YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |0000009E:62F16D0CF54D04<4 | VPMADDWD XMM1,XMM2,[RBP+40h],MASK=K4 |000000A5:62F16D2CF54D02<5 | VPMADDWD YMM1,YMM2,[RBP+40h],MASK=K4 |000000AC:62F16D4CF54D01<6 | VPMADDWD ZMM1,ZMM2,[RBP+40h],MASK=K4 |000000B3:C5E9F6CB | VPSADBW XMM1,XMM2,XMM3 |000000B7:C5EDF6CB | VPSADBW YMM1,YMM2,YMM3 |000000BB:C4E169F6CB | VPSADBW XMM1,XMM2,XMM3,PREFIX=VEX3 |000000C0:C4E16DF6CB | VPSADBW YMM1,YMM2,YMM3,PREFIX=VEX3 |000000C5:62F16D08F6CB | VPSADBW XMM1,XMM2,XMM3,PREFIX=EVEX |000000CB:62F16D28F6CB | VPSADBW YMM1,YMM2,YMM3,PREFIX=EVEX |000000D1:62F16D48F6CB | VPSADBW ZMM1,ZMM2,ZMM3 |000000D7:C5E9F64D40 | VPSADBW XMM1,XMM2,[RBP+40h] |000000DC:C5EDF64D40 | VPSADBW YMM1,YMM2,[RBP+40h] |000000E1:C4E169F64D40 | VPSADBW XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |000000E7:C4E16DF64D40 | VPSADBW YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |000000ED:62F16D08F64D04<4 | VPSADBW XMM1,XMM2,[RBP+40h],PREFIX=EVEX |000000F4:62F16D28F64D02<5 | VPSADBW YMM1,YMM2,[RBP+40h],PREFIX=EVEX |000000FB:62F16D48F64D01<6 | VPSADBW ZMM1,ZMM2,[RBP+40h] | |ENDPROGRAM t5642`

Expected messages t5642.out
  `I0180 Assembling source file "t5642.htm". I0270 Assembling source "t5642". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5642". "t5642.htm"{55} I0510 Assembling program pass 1. "t5642.htm"{55} I0530 Assembling program pass 2 - final. "t5642.htm"{55} I0660 16bit TINY BIN file "t5642.bin" created, size=258. "t5642.htm"{102} I0650 Program "t5642" assembled in 2 passes with errorlevel 0. "t5642.htm"{102} I0750 Source "t5642" (120 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5642.htm.lst" created, size=3270. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲