| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5650: Machine instructions VANDPS VANDNPS VORPS VXORPS

Tested procedures
  IiyVANDPS IiyVANDNPS IiyVORPS IiyVXORPS

Source & expected listing t5650.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON | |t5650 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5E854CB | VANDPS XMM1,XMM2,XMM3 |00000004:C5EC54CB | VANDPS YMM1,YMM2,YMM3 |00000008:C4E16854CB | VANDPS XMM1,XMM2,XMM3,PREFIX=VEX3 |0000000D:C4E16C54CB | VANDPS YMM1,YMM2,YMM3,PREFIX=VEX3 |00000012:62F16C8C54CB | VANDPS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000018:62F16CAC54CB | VANDPS YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000001E:62F16CCC54CB | VANDPS ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000024:C5E8544D40 | VANDPS XMM1,XMM2,[RBP+40h] |00000029:C5EC544D40 | VANDPS YMM1,YMM2,[RBP+40h] |0000002E:C4E168544D40 | VANDPS XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000034:C4E16C544D40 | VANDPS YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |0000003A:62F16C8C544D04<4 | VANDPS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000041:62F16CAC544D02<5 | VANDPS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000048:62F16CCC544D01<6 | VANDPS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000004F:62F16C9C544D10<2 | VANDPS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |00000056:62F16CBC544D10<2 | VANDPS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |0000005D:62F16CDC544D10<2 | VANDPS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |00000064:C5E855CB | VANDNPS XMM1,XMM2,XMM3 |00000068:C5EC55CB | VANDNPS YMM1,YMM2,YMM3 |0000006C:C4E16855CB | VANDNPS XMM1,XMM2,XMM3,PREFIX=VEX3 |00000071:C4E16C55CB | VANDNPS YMM1,YMM2,YMM3,PREFIX=VEX3 |00000076:62F16C8C55CB | VANDNPS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |0000007C:62F16CAC55CB | VANDNPS YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000082:62F16CCC55CB | VANDNPS ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000088:C5E8554D40 | VANDNPS XMM1,XMM2,[RBP+40h] |0000008D:C5EC554D40 | VANDNPS YMM1,YMM2,[RBP+40h] |00000092:C4E168554D40 | VANDNPS XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000098:C4E16C554D40 | VANDNPS YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |0000009E:62F16C8C554D04<4 | VANDNPS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000A5:62F16CAC554D02<5 | VANDNPS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000AC:62F16CCC554D01<6 | VANDNPS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000B3:62F16C9C554D10<2 | VANDNPS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000BA:62F16CBC554D10<2 | VANDNPS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000C1:62F16CDC554D10<2 | VANDNPS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000C8:C5E856CB | VORPS XMM1,XMM2,XMM3 |000000CC:C5EC56CB | VORPS YMM1,YMM2,YMM3 |000000D0:C4E16856CB | VORPS XMM1,XMM2,XMM3,PREFIX=VEX3 |000000D5:C4E16C56CB | VORPS YMM1,YMM2,YMM3,PREFIX=VEX3 |000000DA:62F16C8C56CB | VORPS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |000000E0:62F16CAC56CB | VORPS YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |000000E6:62F16CCC56CB | VORPS ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |000000EC:C5E8564D40 | VORPS XMM1,XMM2,[RBP+40h] |000000F1:C5EC564D40 | VORPS YMM1,YMM2,[RBP+40h] |000000F6:C4E168564D40 | VORPS XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |000000FC:C4E16C564D40 | VORPS YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |00000102:62F16C8C564D04<4 | VORPS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000109:62F16CAC564D02<5 | VORPS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000110:62F16CCC564D01<6 | VORPS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000117:62F16C9C564D10<2 | VORPS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |0000011E:62F16CBC564D10<2 | VORPS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |00000125:62F16CDC564D10<2 | VORPS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |0000012C:C5E857CB | VXORPS XMM1,XMM2,XMM3 |00000130:C5EC57CB | VXORPS YMM1,YMM2,YMM3 |00000134:C4E16857CB | VXORPS XMM1,XMM2,XMM3,PREFIX=VEX3 |00000139:C4E16C57CB | VXORPS YMM1,YMM2,YMM3,PREFIX=VEX3 |0000013E:62F16C8C57CB | VXORPS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000144:62F16CAC57CB | VXORPS YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000014A:62F16CCC57CB | VXORPS ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000150:C5E8574D40 | VXORPS XMM1,XMM2,[RBP+40h] |00000155:C5EC574D40 | VXORPS YMM1,YMM2,[RBP+40h] |0000015A:C4E168574D40 | VXORPS XMM1,XMM2,[RBP+40h],PREFIX=VEX3 |00000160:C4E16C574D40 | VXORPS YMM1,YMM2,[RBP+40h],PREFIX=VEX3 |00000166:62F16C8C574D04<4 | VXORPS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000016D:62F16CAC574D02<5 | VXORPS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000174:62F16CCC574D01<6 | VXORPS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000017B:62F16C9C574D10<2 | VXORPS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |00000182:62F16CBC574D10<2 | VXORPS YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |00000189:62F16CDC574D10<2 | VXORPS ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON | |ENDPROGRAM t5650`

Expected messages t5650.out
  `I0180 Assembling source file "t5650.htm". I0270 Assembling source "t5650". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5650". "t5650.htm"{58} I0510 Assembling program pass 1. "t5650.htm"{58} I0530 Assembling program pass 2 - final. "t5650.htm"{58} I0660 16bit TINY BIN file "t5650.bin" created, size=400. "t5650.htm"{128} I0650 Program "t5650" assembled in 2 passes with errorlevel 0. "t5650.htm"{128} I0750 Source "t5650" (146 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5650.htm.lst" created, size=5144. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲