| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4670: Machine instructions VFMADDSS VFMADDSD VFMSUBSS VFMSUBSD

Tested procedures
  IiaVFMADDSS IiaVFMADDSD IiaVFMSUBSS IiaVFMSUBSD

Source & expected listing t4670.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,SIMD=AVX,FMA=ON,AMD=ON | |t4670 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E3696A0E40 | VFMADDSS XMM1,XMM2,[RSI],XMM4 |00000006:C4E3696B0E40 | VFMADDSD XMM1,XMM2,[RSI],XMM4 |0000000C:C4E3696E0E40 | VFMSUBSS XMM1,XMM2,[RSI],XMM4 |00000012:C4E3696F0E40 | VFMSUBSD XMM1,XMM2,[RSI],XMM4 |00000018:C4E3E96A0E30 | VFMADDSS XMM1,XMM2,XMM3,[RSI] |0000001E:C4E3E96B0E30 | VFMADDSD XMM1,XMM2,XMM3,[RSI] |00000024:C4E3E96E0E30 | VFMSUBSS XMM1,XMM2,XMM3,[RSI] |0000002A:C4E3E96F0E30 | VFMSUBSD XMM1,XMM2,XMM3,[RSI] |00000030:C4E3696ACB40 | VFMADDSS XMM1,XMM2,XMM3,XMM4 |00000036:C4E3696BCB40 | VFMADDSD XMM1,XMM2,XMM3,XMM4 |0000003C:C4E3696ECB40 | VFMSUBSS XMM1,XMM2,XMM3,XMM4 |00000042:C4E3696FCB40 | VFMSUBSD XMM1,XMM2,XMM3,XMM4 |00000048:C4E3E96ACC30 | VFMADDSS XMM1,XMM2,XMM3,XMM4,CODE=LONG |0000004E:C4E3E96BCC30 | VFMADDSD XMM1,XMM2,XMM3,XMM4,CODE=LONG |00000054:C4E3E96ECC30 | VFMSUBSS XMM1,XMM2,XMM3,XMM4,CODE=LONG |0000005A:C4E3E96FCC30 | VFMSUBSD XMM1,XMM2,XMM3,XMM4,CODE=LONG | |ENDPROGRAM t4670`

Expected messages t4670.out
  `I0180 Assembling source file "t4670.htm". I0270 Assembling source "t4670". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4670". "t4670.htm"{58} I0510 Assembling program pass 1. "t4670.htm"{58} I0530 Assembling program pass 2 - final. "t4670.htm"{58} I0660 16bit TINY BIN file "t4670.bin" created, size=96. "t4670.htm"{76} I0650 Program "t4670" assembled in 2 passes with errorlevel 0. "t4670.htm"{76} I0750 Source "t4670" (94 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4670.htm.lst" created, size=1209. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲