| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5403: Machine instructions VFNMADD312SS VFNMADD123SS VFNMADD321SS VFNMSUB312SS VFNMSUB123SS VFNMSUB321SS

Tested procedures
  IibVFNMADD312SS IibVFNMADD123SS IibVFNMADD321SS IibVFNMSUB312SS IibVFNMSUB123SS IibVFNMSUB321SS

Source & expected listing t5403.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,DUMPALL=OFF,CPU=X64,SIMD=AVX512,FMA=ON,EVEX=ON | |t5403 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E2699DCB | VFNMADD312SS XMM1,XMM2,XMM3 |00000005:62F26D589DCB | VFNMADD312SS XMM1,XMM2,XMM3,ROUND=UP |0000000B:62F26D8C9DCB | VFNMADD312SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000011:62F26D8C9D4D10<2 | VFNMADD312SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000018:C4E269ADCB | VFNMADD123SS XMM1,XMM2,XMM3 |0000001D:62F26D58ADCB | VFNMADD123SS XMM1,XMM2,XMM3,ROUND=UP |00000023:62F26D8CADCB | VFNMADD123SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000029:62F26D8CAD4D10<2 | VFNMADD123SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000030:C4E269BDCB | VFNMADD321SS XMM1,XMM2,XMM3 |00000035:62F26D58BDCB | VFNMADD321SS XMM1,XMM2,XMM3,ROUND=UP |0000003B:62F26D8CBDCB | VFNMADD321SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000041:62F26D8CBD4D10<2 | VFNMADD321SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000048:C4E2699FCB | VFNMSUB312SS XMM1,XMM2,XMM3 |0000004D:62F26D589FCB | VFNMSUB312SS XMM1,XMM2,XMM3,ROUND=UP |00000053:62F26D8C9FCB | VFNMSUB312SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000059:62F26D8C9F4D10<2 | VFNMSUB312SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000060:C4E269AFCB | VFNMSUB123SS XMM1,XMM2,XMM3 |00000065:62F26D58AFCB | VFNMSUB123SS XMM1,XMM2,XMM3,ROUND=UP |0000006B:62F26D8CAFCB | VFNMSUB123SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000071:62F26D8CAF4D10<2 | VFNMSUB123SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000078:C4E269BFCB | VFNMSUB321SS XMM1,XMM2,XMM3 |0000007D:62F26D58BFCB | VFNMSUB321SS XMM1,XMM2,XMM3,ROUND=UP |00000083:62F26D8CBFCB | VFNMSUB321SS XMM1,XMM2,XMM3,MASK=K4,ZEROING=ON |00000089:62F26D8CBF4D10<2 | VFNMSUB321SS XMM1,XMM2,[RBP+40h],MASK=K4,ZEROING=ON | |ENDPROGRAM t5403`

Expected messages t5403.out
  `I0180 Assembling source file "t5403.htm". I0270 Assembling source "t5403". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5403". "t5403.htm"{64} I0510 Assembling program pass 1. "t5403.htm"{64} I0530 Assembling program pass 2 - final. "t5403.htm"{64} I0660 16bit TINY BIN file "t5403.bin" created, size=144. "t5403.htm"{90} I0650 Program "t5403" assembled in 2 passes with errorlevel 0. "t5403.htm"{90} I0750 Source "t5403" (108 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5403.htm.lst" created, size=2184. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲