| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3505: Machine instructions FNENI FENI FNDISI FDISI FNCLEX FCLEX FNINIT FINIT FSETPM FNSETPM FRSTPM

Tested procedures
  IifFNENI IifFENI IifFNDISI IifFDISI IifFNCLEX IifFCLEX IifFNINIT IifFINIT IifFSETPM IifFNSETPM IifFRSTPM

Source & expected listing t3505.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=24,CPU=X64,FPU=ON | |t3505 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:DBE0 | FNENI |0002:9BDBE0 | FENI |0005:DBE1 | FNDISI |0007:9BDBE1 | FDISI |000A:DBE2 | FNCLEX |000C:9BDBE2 | FCLEX |000F:DBE3 | FNINIT |0011:9BDBE3 | FINIT | | EUROASM UNDOC=ENABLE, PROT=ENABLE |0014:9BDBE4 | FSETPM |0017:DBE4 | FNSETPM |0019:DBE5 | FRSTPM |001B:DBF4 | FRSTPM CODE=LONG |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:DBE0 | FNENI |00000002:9BDBE0 | FENI |00000005:DBE1 | FNDISI |00000007:9BDBE1 | FDISI |0000000A:DBE2 | FNCLEX |0000000C:9BDBE2 | FCLEX |0000000F:DBE3 | FNINIT |00000011:9BDBE3 | FINIT |00000014:9BDBE4 | FSETPM |00000017:DBE4 | FNSETPM |00000019:DBE5 | FRSTPM |0000001B:DBF4 | FRSTPM CODE=LONG |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:DBE0 | FNENI |00000002:9BDBE0 | FENI |00000005:DBE1 | FNDISI |00000007:9BDBE1 | FDISI |0000000A:DBE2 | FNCLEX |0000000C:9BDBE2 | FCLEX |0000000F:DBE3 | FNINIT |00000011:9BDBE3 | FINIT |00000014:9BDBE4 | FSETPM |00000017:DBE4 | FNSETPM |00000019:DBE5 | FRSTPM |0000001B:DBF4 | FRSTPM CODE=LONG | |ENDPROGRAM t3505`

Expected messages t3505.out
  `I0180 Assembling source file "t3505.htm". I0270 Assembling source "t3505". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3505". "t3505.htm"{79} I0510 Assembling program pass 1. "t3505.htm"{79} I0530 Assembling program pass 2 - final. "t3505.htm"{79} I0660 16bit TINY BIN file "t3505.bin" created, size=93. "t3505.htm"{120} I0650 Program "t3505" assembled in 2 passes with errorlevel 0. "t3505.htm"{120} I0750 Source "t3505" (138 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3505.htm.lst" created, size=1656. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲