| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3635: Machine instructions POR PADDSB PADDSW PMAXSW PXOR PMULUDQ PMADDWD PSADBW

Tested procedures
  IimGroupSSE2 IimPOR IimPADDSB IimPADDSW IimPMAXSW IimPXOR IimPMULUDQ IimPMADDWD IimPSADBW

Source & expected listing t3635.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=30, CPU=X64, MMX=ON, SIMD=SSE2 | |t3635 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF, IMAGEBASE=0 |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:0FEBCF | POR MM1,MM7 |0003:260FEB14 | POR MM2,[ES:SI] |0007:660FEBCF | POR XMM1,XMM7 |000B:660FEB56F8 | POR XMM2,[BP-8] |0010:0FECCF | PADDSB MM1,MM7 |0013:260FEC14 | PADDSB MM2,[ES:SI] |0017:660FECCF | PADDSB XMM1,XMM7 |001B:660FEC56F8 | PADDSB XMM2,[BP-8] |0020:0FEDCF | PADDSW MM1,MM7 |0023:260FED14 | PADDSW MM2,[ES:SI] |0027:660FEDCF | PADDSW XMM1,XMM7 |002B:660FED56F8 | PADDSW XMM2,[BP-8] |0030:0FEECF | PMAXSW MM1,MM7 |0033:260FEE14 | PMAXSW MM2,[ES:SI] |0037:660FEECF | PMAXSW XMM1,XMM7 |003B:660FEE56F8 | PMAXSW XMM2,[BP-8] |0040:0FEFCF | PXOR MM1,MM7 |0043:260FEF14 | PXOR MM2,[ES:SI] |0047:660FEFCF | PXOR XMM1,XMM7 |004B:660FEF56F8 | PXOR XMM2,[BP-8] |0050:0FF4CF | PMULUDQ MM1,MM7 |0053:260FF414 | PMULUDQ MM2,[ES:SI] |0057:660FF4CF | PMULUDQ XMM1,XMM7 |005B:660FF456F8 | PMULUDQ XMM2,[BP-8] |0060:0FF5CF | PMADDWD MM1,MM7 |0063:260FF514 | PMADDWD MM2,[ES:SI] |0067:660FF5CF | PMADDWD XMM1,XMM7 |006B:660FF556F8 | PMADDWD XMM2,[BP-8] |0070:0FF6CF | PSADBW MM1,MM7 |0073:260FF614 | PSADBW MM2,[ES:SI] |0077:660FF6CF | PSADBW XMM1,XMM7 |007B:660FF656F8 | PSADBW XMM2,[BP-8] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0FEBCF | POR MM1,MM7 |00000003:0FEB16 | POR MM2,[ESI] |00000006:660FEBCF | POR XMM1,XMM7 |0000000A:66670FEB56F8 | POR XMM2,[BP-8] |00000010:0FECCF | PADDSB MM1,MM7 |00000013:0FEC16 | PADDSB MM2,[ESI] |00000016:660FECCF | PADDSB XMM1,XMM7 |0000001A:66670FEC56F8 | PADDSB XMM2,[BP-8] |00000020:0FEDCF | PADDSW MM1,MM7 |00000023:0FED16 | PADDSW MM2,[ESI] |00000026:660FEDCF | PADDSW XMM1,XMM7 |0000002A:66670FED56F8 | PADDSW XMM2,[BP-8] |00000030:0FEECF | PMAXSW MM1,MM7 |00000033:0FEE16 | PMAXSW MM2,[ESI] |00000036:660FEECF | PMAXSW XMM1,XMM7 |0000003A:66670FEE56F8 | PMAXSW XMM2,[BP-8] |00000040:0FEFCF | PXOR MM1,MM7 |00000043:0FEF16 | PXOR MM2,[ESI] |00000046:660FEFCF | PXOR XMM1,XMM7 |0000004A:66670FEF56F8 | PXOR XMM2,[BP-8] |00000050:0FF4CF | PMULUDQ MM1,MM7 |00000053:0FF416 | PMULUDQ MM2,[ESI] |00000056:660FF4CF | PMULUDQ XMM1,XMM7 |0000005A:66670FF456F8 | PMULUDQ XMM2,[BP-8] |00000060:0FF5CF | PMADDWD MM1,MM7 |00000063:0FF516 | PMADDWD MM2,[ESI] |00000066:660FF5CF | PMADDWD XMM1,XMM7 |0000006A:66670FF556F8 | PMADDWD XMM2,[BP-8] |00000070:0FF6CF | PSADBW MM1,MM7 |00000073:0FF616 | PSADBW MM2,[ESI] |00000076:660FF6CF | PSADBW XMM1,XMM7 |0000007A:66670FF656F8 | PSADBW XMM2,[BP-8] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0FEBCF | POR MM1,MM7 |00000003:670FEB16 | POR MM2,[ESI] |00000007:660FEBCF | POR XMM1,XMM7 |0000000B:66410FEB542DF8 | POR XMM2,[R13+RBP-8] |00000012:0FECCF | PADDSB MM1,MM7 |00000015:670FEC16 | PADDSB MM2,[ESI] |00000019:660FECCF | PADDSB XMM1,XMM7 |0000001D:66410FEC542DF8 | PADDSB XMM2,[R13+RBP-8] |00000024:0FEDCF | PADDSW MM1,MM7 |00000027:670FED16 | PADDSW MM2,[ESI] |0000002B:660FEDCF | PADDSW XMM1,XMM7 |0000002F:66410FED542DF8 | PADDSW XMM2,[R13+RBP-8] |00000036:0FEECF | PMAXSW MM1,MM7 |00000039:670FEE16 | PMAXSW MM2,[ESI] |0000003D:660FEECF | PMAXSW XMM1,XMM7 |00000041:66410FEE542DF8 | PMAXSW XMM2,[R13+RBP-8] |00000048:0FEFCF | PXOR MM1,MM7 |0000004B:670FEF16 | PXOR MM2,[ESI] |0000004F:660FEFCF | PXOR XMM1,XMM7 |00000053:66410FEF542DF8 | PXOR XMM2,[R13+RBP-8] |0000005A:0FF4CF | PMULUDQ MM1,MM7 |0000005D:670FF416 | PMULUDQ MM2,[ESI] |00000061:660FF4CF | PMULUDQ XMM1,XMM7 |00000065:66410FF4542DF8 | PMULUDQ XMM2,[R13+RBP-8] |0000006C:0FF5CF | PMADDWD MM1,MM7 |0000006F:670FF516 | PMADDWD MM2,[ESI] |00000073:660FF5CF | PMADDWD XMM1,XMM7 |00000077:66410FF5542DF8 | PMADDWD XMM2,[R13+RBP-8] |0000007E:0FF6CF | PSADBW MM1,MM7 |00000081:670FF616 | PSADBW MM2,[ESI] |00000085:660FF6CF | PSADBW XMM1,XMM7 |00000089:66410FF6542DF8 | PSADBW XMM2,[R13+RBP-8] | |ENDPROGRAM t3635`

Expected messages t3635.out
  `I0180 Assembling source file "t3635.htm". I0270 Assembling source "t3635". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3635". "t3635.htm"{73} I0510 Assembling program pass 1. "t3635.htm"{73} I0530 Assembling program pass 2 - final. "t3635.htm"{73} I0660 16bit TINY BIN file "t3635.bin" created, size=400. "t3635.htm"{173} I0650 Program "t3635" assembled in 2 passes with errorlevel 0. "t3635.htm"{173} I0750 Source "t3635" (191 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3635.htm.lst" created, size=5181. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲