| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3795: Machine instructions PMOVSXBW PMOVSXBD PMOVSXBQ PMOVSXWD PMOVSXWQ PMOVSXDQ

Tested procedures
  IipGroupSSE4_1 IipPMOVSXBW IipPMOVSXBD IipPMOVSXBQ IipPMOVSXWD IipPMOVSXWQ IipPMOVSXDQ

Source & expected listing t3795.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=32, CPU=X64, SIMD=SSE4.1 | |t3795 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:660F3820CF | PMOVSXBW XMM1,XMM7 |0005:660F38200C | PMOVSXBW XMM1,[SI] |000A:660F3821CF | PMOVSXBD XMM1,XMM7 |000F:660F38210C | PMOVSXBD XMM1,[SI] |0014:660F3822CF | PMOVSXBQ XMM1,XMM7 |0019:660F38220C | PMOVSXBQ XMM1,[SI] |001E:660F3823CF | PMOVSXWD XMM1,XMM7 |0023:660F38230C | PMOVSXWD XMM1,[SI] |0028:660F3824CF | PMOVSXWQ XMM1,XMM7 |002D:660F38240C | PMOVSXWQ XMM1,[SI] |0032:660F3825CF | PMOVSXDQ XMM1,XMM7 |0037:660F38250C | PMOVSXDQ XMM1,[SI] |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660F3820CF | PMOVSXBW XMM1,XMM7 |00000005:660F38200E | PMOVSXBW XMM1,[ESI] |0000000A:660F3821CF | PMOVSXBD XMM1,XMM7 |0000000F:660F38210E | PMOVSXBD XMM1,[ESI] |00000014:660F3822CF | PMOVSXBQ XMM1,XMM7 |00000019:660F38220E | PMOVSXBQ XMM1,[ESI] |0000001E:660F3823CF | PMOVSXWD XMM1,XMM7 |00000023:660F38230E | PMOVSXWD XMM1,[ESI] |00000028:660F3824CF | PMOVSXWQ XMM1,XMM7 |0000002D:660F38240E | PMOVSXWQ XMM1,[ESI] |00000032:660F3825CF | PMOVSXDQ XMM1,XMM7 |00000037:66670F38250C | PMOVSXDQ XMM1,[SI] |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:66410F3820CB | PMOVSXBW XMM1,XMM11 |00000006:66450F3820CB | PMOVSXBW XMM9,XMM11 |0000000C:660F38200E | PMOVSXBW XMM1,[RSI] |00000011:660F3821CF | PMOVSXBD XMM1,XMM7 |00000016:66450F3821CB | PMOVSXBD XMM9,XMM11 |0000001C:66670F38210E | PMOVSXBD XMM1,[ESI] |00000022:660F3822CF | PMOVSXBQ XMM1,XMM7 |00000027:66440F3822CF | PMOVSXBQ XMM9,XMM7 |0000002D:6667420F38220C0E | PMOVSXBQ XMM1,[ESI+R9D] |00000035:660F3823CF | PMOVSXWD XMM1,XMM7 |0000003A:66450F3823CB | PMOVSXWD XMM9,XMM11 |00000040:660F38230C2500000000 | PMOVSXWD XMM1,[0] |0000004A:660F3824CF | PMOVSXWQ XMM1,XMM7 |0000004F:66440F38240E | PMOVSXWQ XMM9,[RSI] |00000055:660F3825CF | PMOVSXDQ XMM1,XMM7 |0000005A:66460F38255C4E10 | PMOVSXDQ XMM11,[RSI+2*R9+16] | |ENDPROGRAM t3795`

Expected messages t3795.out
  `I0180 Assembling source file "t3795.htm". I0270 Assembling source "t3795". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3795". "t3795.htm"{67} I0510 Assembling program pass 1. "t3795.htm"{67} I0530 Assembling program pass 2 - final. "t3795.htm"{67} I0660 16bit TINY BIN file "t3795.bin" created, size=226. "t3795.htm"{111} I0650 Program "t3795" assembled in 2 passes with errorlevel 0. "t3795.htm"{111} I0750 Source "t3795" (129 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3795.htm.lst" created, size=2601. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲