| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4520: Machine instructions VPMACSSWW VPMACSSWD VPMACSSDQL VPMACSSDD VPMACSSDQH

Tested procedures
  IixVPMACSSWW IixVPMACSSWD IixVPMACSSDQL IixVPMACSSDD IixVPMACSSDQH

Source & expected listing t4520.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=28,CPU=X64,SIMD=AVX,AMD=ON,XOP=ON,PROT=ON | |t4520 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:8FE86885CB40 | VPMACSSWW XMM1,XMM2,XMM3,XMM4 |00000006:8FE868850E40 | VPMACSSWW XMM1,XMM2,[RSI],XMM4 |0000000C:8FE86886CB40 | VPMACSSWD XMM1,XMM2,XMM3,XMM4 |00000012:8FE868860E40 | VPMACSSWD XMM1,XMM2,[RSI],XMM4 |00000018:8FE86887CB40 | VPMACSSDQL XMM1,XMM2,XMM3,XMM4 |0000001E:8FE868870E40 | VPMACSSDQL XMM1,XMM2,[RSI],XMM4 |00000024:8FE8688ECB40 | VPMACSSDD XMM1,XMM2,XMM3,XMM4 |0000002A:8FE8688E0E40 | VPMACSSDD XMM1,XMM2,[RSI],XMM4 |00000030:8FE8688FCB40 | VPMACSSDQH XMM1,XMM2,XMM3,XMM4 |00000036:8FE8688F0E40 | VPMACSSDQH XMM1,XMM2,[RSI],XMM4 |0000003C:8F48288FCBC0 | VPMACSSDQH XMM9,XMM10,XMM11,XMM12 |00000042:678FA8688F0C4640 | VPMACSSDQH XMM1,XMM2,[ESI+2*R8D],XMM4 | | ENDPROGRAM t4520`

Expected messages t4520.out
  `I0180 Assembling source file "t4520.htm". I0270 Assembling source "t4520". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4520". "t4520.htm"{61} I0510 Assembling program pass 1. "t4520.htm"{61} I0530 Assembling program pass 2 - final. "t4520.htm"{61} I0660 16bit TINY BIN file "t4520.bin" created, size=74. "t4520.htm"{75} I0650 Program "t4520" assembled in 2 passes with errorlevel 0. "t4520.htm"{75} I0750 Source "t4520" (93 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4520.htm.lst" created, size=1054. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲