| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5762: Machine instructions VPTESTNMB VPTESTNMW VPTESTNMD VPTESTNMQ

Tested procedures
  IiyVPTESTNMB IiyVPTESTNMW IiyVPTESTNMD IiyVPTESTNMQ

Source & expected listing t5762.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON | |t5762 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F26E0C26CB | VPTESTNMB K1,XMM2,XMM3,MASK=K4 |00000006:62F26E2C26CB | VPTESTNMB K1,YMM2,YMM3,MASK=K4 |0000000C:62F26E4C26CB | VPTESTNMB K1,ZMM2,ZMM3,MASK=K4 |00000012:62F26E0C264D04<4 | VPTESTNMB K1,XMM2,[RBP+40h],MASK=K4 |00000019:62F26E2C264D02<5 | VPTESTNMB K1,YMM2,[RBP+40h],MASK=K4 |00000020:62F26E4C264D01<6 | VPTESTNMB K1,ZMM2,[RBP+40h],MASK=K4 |00000027:62F2EE0C26CB | VPTESTNMW K1,XMM2,XMM3,MASK=K4 |0000002D:62F2EE2C26CB | VPTESTNMW K1,YMM2,YMM3,MASK=K4 |00000033:62F2EE4C26CB | VPTESTNMW K1,ZMM2,ZMM3,MASK=K4 |00000039:62F2EE0C264D04<4 | VPTESTNMW K1,XMM2,[RBP+40h],MASK=K4 |00000040:62F2EE2C264D02<5 | VPTESTNMW K1,YMM2,[RBP+40h],MASK=K4 |00000047:62F2EE4C264D01<6 | VPTESTNMW K1,ZMM2,[RBP+40h],MASK=K4 |0000004E:62F26E0C27CB | VPTESTNMD K1,XMM2,XMM3,MASK=K4 |00000054:62F26E2C27CB | VPTESTNMD K1,YMM2,YMM3,MASK=K4 |0000005A:62F26E4C27CB | VPTESTNMD K1,ZMM2,ZMM3,MASK=K4 |00000060:62F26E0C274D04<4 | VPTESTNMD K1,XMM2,[RBP+40h],MASK=K4 |00000067:62F26E2C274D02<5 | VPTESTNMD K1,YMM2,[RBP+40h],MASK=K4 |0000006E:62F26E4C274D01<6 | VPTESTNMD K1,ZMM2,[RBP+40h],MASK=K4 |00000075:62F26E1C274D10<2 | VPTESTNMD K1,XMM2,[RBP+40h],MASK=K4,BCST=ON |0000007C:62F26E3C274D10<2 | VPTESTNMD K1,YMM2,[RBP+40h],MASK=K4,BCST=ON |00000083:62F26E5C274D10<2 | VPTESTNMD K1,ZMM2,[RBP+40h],MASK=K4,BCST=ON |0000008A:62F2EE0C27CB | VPTESTNMQ K1,XMM2,XMM3,MASK=K4 |00000090:62F2EE2C27CB | VPTESTNMQ K1,YMM2,YMM3,MASK=K4 |00000096:62F2EE4C27CB | VPTESTNMQ K1,ZMM2,ZMM3,MASK=K4 |0000009C:62F2EE0C274D04<4 | VPTESTNMQ K1,XMM2,[RBP+40h],MASK=K4 |000000A3:62F2EE2C274D02<5 | VPTESTNMQ K1,YMM2,[RBP+40h],MASK=K4 |000000AA:62F2EE4C274D01<6 | VPTESTNMQ K1,ZMM2,[RBP+40h],MASK=K4 |000000B1:62F2EE1C274D08<3 | VPTESTNMQ K1,XMM2,[RBP+40h],MASK=K4,BCST=ON |000000B8:62F2EE3C274D08<3 | VPTESTNMQ K1,YMM2,[RBP+40h],MASK=K4,BCST=ON |000000BF:62F2EE5C274D08<3 | VPTESTNMQ K1,ZMM2,[RBP+40h],MASK=K4,BCST=ON | |ENDPROGRAM t5762`

Expected messages t5762.out
  `I0180 Assembling source file "t5762.htm". I0270 Assembling source "t5762". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5762". "t5762.htm"{58} I0510 Assembling program pass 1. "t5762.htm"{58} I0530 Assembling program pass 2 - final. "t5762.htm"{58} I0660 16bit TINY BIN file "t5762.bin" created, size=198. "t5762.htm"{90} I0650 Program "t5762" assembled in 2 passes with errorlevel 0. "t5762.htm"{90} I0750 Source "t5762" (108 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5762.htm.lst" created, size=2329. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲