| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5608: Machine instructions VPMAXSB VPMAXSQ VPMAXSD VPMAXSQ

Tested procedures
  IizVPMAXSB IizVPMAXSQ IizVPMAXSD

Source & expected listing t5608.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5608 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C4E2693CCB | VPMAXSB XMM1,XMM2,XMM3 |00000005:C4E26D3CCB | VPMAXSB YMM1,YMM2,YMM3 |0000000A:62F26D0C3CCB | VPMAXSB XMM1,XMM2,XMM3,MASK=K4 |00000010:62F26DAC3CCB | VPMAXSB YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000016:62F26DCC3CCB | VPMAXSB ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |0000001C:C4E2693C4D40 | VPMAXSB XMM1,XMM2,[RBP+40h] |00000022:C4E26D3C4D40 | VPMAXSB YMM1,YMM2,[RBP+40h] |00000028:62F26D483C4D01<6 | VPMAXSB ZMM1,ZMM2,[RBP+40h] |0000002F:62F26D0C3C4D04<4 | VPMAXSB XMM1,XMM2,[RBP+40h],MASK=K4 |00000036:62F26DCC3C4D01<6 | VPMAXSB ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000003D:C5E9EECB | VPMAXSW XMM1,XMM2,XMM3 |00000041:C5EDEECB | VPMAXSW YMM1,YMM2,YMM3 |00000045:62F16D0CEECB | VPMAXSW XMM1,XMM2,XMM3,MASK=K4 |0000004B:62F16DACEECB | VPMAXSW YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000051:62F16DCCEECB | VPMAXSW ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000057:C5E9EE4D40 | VPMAXSW XMM1,XMM2,[RBP+40h] |0000005C:C5EDEE4D40 | VPMAXSW YMM1,YMM2,[RBP+40h] |00000061:62F16D48EE4D01<6 | VPMAXSW ZMM1,ZMM2,[RBP+40h] |00000068:62F16D0CEE4D04<4 | VPMAXSW XMM1,XMM2,[RBP+40h],MASK=K4 |0000006F:62F16DACEE4D02<5 | VPMAXSW YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON |00000076:62F16DCCEE4D01<6 | VPMAXSW ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |0000007D:C4E2693DCB | VPMAXSD XMM1,XMM2,XMM3 |00000082:C4E26D3DCB | VPMAXSD YMM1,YMM2,YMM3 |00000087:62F26D0C3DCB | VPMAXSD XMM1,XMM2,XMM3,MASK=K4 |0000008D:62F26DAC3DCB | VPMAXSD YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |00000093:62F26DCC3DCB | VPMAXSD ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000099:62F269283DCB | VPMAXSD ZMM1,ZMM2,ZMM3,EH=0,OPER=2 ; MVEX swizzle {badc}. |0000009F:C4E2693D4D40 | VPMAXSD XMM1,XMM2,[RBP+40h] |000000A5:C4E26D3D4D40 | VPMAXSD YMM1,YMM2,[RBP+40h] |000000AB:62F26D483D4D01<6 | VPMAXSD ZMM1,ZMM2,[RBP+40h] |000000B2:62F26D183D4D10<2 | VPMAXSD XMM1,XMM2,[RBP+40h],BCST=ON |000000B9:62F26D383D4D10<2 | VPMAXSD YMM1,YMM2,[RBP+40h],BCST=ON |000000C0:62F26D583D4D10<2 | VPMAXSD ZMM1,ZMM2,[RBP+40h],BCST=ON |000000C7:62F26D0C3D4D04<4 | VPMAXSD XMM1,XMM2,[RBP+40h],MASK=K4 |000000CE:62F26D1C3D4D10<2 | VPMAXSD XMM1,XMM2,[RBP+40h],MASK=K4,BCST=ON |000000D5:62F26DBC3D4D10<2 | VPMAXSD YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |000000DC:62F26DCC3D4D01<6 | VPMAXSD ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON |000000E3:62F269083D4D01<6 | VPMAXSD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=0 ; {16to16}. |000000EA:62F269183D4D10<2 | VPMAXSD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=1 ; {1to16}. |000000F1:62F269283D4D04<4 | VPMAXSD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=2 ; {4to16}. |000000F8:62F269483D4D04<4 | VPMAXSD ZMM1,ZMM2,[RBP+40h],PREFIX=MVEX,OPER=4 ; {uint8}. |000000FF:62F2ED083DCB | VPMAXSQ XMM1,XMM2,XMM3 |00000105:62F2EDAC3DCB | VPMAXSQ YMM1,YMM2,YMM3,MASK=K4,ZEROING=ON |0000010B:62F2EDCC3DCB | VPMAXSQ ZMM1,ZMM2,ZMM3,MASK=K4,ZEROING=ON |00000111:62F2ED083D4D04<4 | VPMAXSQ XMM1,XMM2,[RBP+40h] |00000118:62F2ED283D4D02<5 | VPMAXSQ YMM1,YMM2,[RBP+40h] |0000011F:62F2ED483D4D01<6 | VPMAXSQ ZMM1,ZMM2,[RBP+40h] |00000126:62F2ED183D4D08<3 | VPMAXSQ XMM1,XMM2,[RBP+40h],BCST=ON |0000012D:62F2ED383D4D08<3 | VPMAXSQ YMM1,YMM2,[RBP+40h],BCST=ON |00000134:62F2ED583D4D08<3 | VPMAXSQ ZMM1,ZMM2,[RBP+40h],BCST=ON |0000013B:62F2ED0C3D4D04<4 | VPMAXSQ XMM1,XMM2,[RBP+40h],MASK=K4 |00000142:62F2ED1C3D4D08<3 | VPMAXSQ XMM1,XMM2,[RBP+40h],MASK=K4,BCST=ON |00000149:62F2EDBC3D4D08<3 | VPMAXSQ YMM1,YMM2,[RBP+40h],MASK=K4,ZEROING=ON,BCST=ON |00000150:62F2EDCC3D4D01<6 | VPMAXSQ ZMM1,ZMM2,[RBP+40h],MASK=K4,ZEROING=ON | |ENDPROGRAM t5608`

Expected messages t5608.out
  `I0180 Assembling source file "t5608.htm". I0270 Assembling source "t5608". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5608". "t5608.htm"{55} I0510 Assembling program pass 1. "t5608.htm"{55} I0530 Assembling program pass 2 - final. "t5608.htm"{55} I0660 16bit TINY BIN file "t5608.bin" created, size=343. "t5608.htm"{111} I0650 Program "t5608" assembled in 2 passes with errorlevel 0. "t5608.htm"{111} I0750 Source "t5608" (129 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5608.htm.lst" created, size=4046. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲