| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3820: Machine instructions DPPS DPPD MPSADBW PCMPESTRM PCMPESTRI PCMPISTRM PCMPISTRI

Tested procedures
  IipGroupSSE4 IipDPPS IipDPPD IipMPSADBW IipPCMPESTRM IipPCMPESTRI IipPCMPISTRM IipPCMPISTRI

Source & expected listing t3820.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,CPU=X64,SIMD=SSE4.2 | |t3820 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:660F3A40CF01 | DPPS XMM1,XMM7,1 |0006:660F3A400C01 | DPPS XMM1,[SI],1 |000C:660F3A41CF01 | DPPD XMM1,XMM7,1 |0012:660F3A410C01 | DPPD XMM1,[SI],1 |0018:660F3A42CF01 | MPSADBW XMM1,XMM7,1 |001E:660F3A420C01 | MPSADBW XMM1,[SI],1 |0024:660F3A60CF01 | PCMPESTRM XMM1,XMM7,1 |002A:660F3A600C01 | PCMPESTRM XMM1,[SI],1 |0030:660F3A61CF01 | PCMPESTRI XMM1,XMM7,1 |0036:660F3A610E000001 | PCMPESTRI XMM1,[0],1 |003E:660F3A62CF01 | PCMPISTRM XMM1,XMM7,1 |0044:66670F3A620E01 | PCMPISTRM XMM1,[ESI],1 |004B:660F3A63CF01 | PCMPISTRI XMM1,XMM7,1 |0051:26660F3A630C01 | PCMPISTRI XMM1,[ES:SI],1 |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:660F3A40CF01 | DPPS XMM1,XMM7,1 |00000006:660F3A400E01 | DPPS XMM1,[ESI],1 |0000000C:660F3A41CF01 | DPPD XMM1,XMM7,1 |00000012:660F3A410E01 | DPPD XMM1,[ESI],1 |00000018:660F3A42CF01 | MPSADBW XMM1,XMM7,1 |0000001E:660F3A420E01 | MPSADBW XMM1,[ESI],1 |00000024:660F3A60CF01 | PCMPESTRM XMM1,XMM7,1 |0000002A:660F3A600E01 | PCMPESTRM XMM1,[ESI],1 |00000030:660F3A61CF01 | PCMPESTRI XMM1,XMM7,1 |00000036:660F3A610E01 | PCMPESTRI XMM1,[ESI],1 |0000003C:660F3A62CF01 | PCMPISTRM XMM1,XMM7,1 |00000042:660F3A620D0000000001 | PCMPISTRM XMM1,[0],1 |0000004C:660F3A63CF01 | PCMPISTRI XMM1,XMM7,1 |00000052:66670F3A630C01 | PCMPISTRI XMM1,[SI],1 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:660F3A40CF01 | DPPS XMM1,XMM7,1 |00000006:660F3A400E01 | DPPS XMM1,[RSI],1 |0000000C:660F3A41CF01 | DPPD XMM1,XMM7,1 |00000012:660F3A410E01 | DPPD XMM1,[RSI],1 |00000018:660F3A42CF01 | MPSADBW XMM1,XMM7,1 |0000001E:660F3A420E01 | MPSADBW XMM1,[RSI],1 |00000024:660F3A60CF01 | PCMPESTRM XMM1,XMM7,1 |0000002A:660F3A60CF01 | PCMPESTRM XMM1,XMM7,1,DATA=DWORD |00000030:66480F3A60CF01 | PCMPESTRM XMM1,XMM7,1,DATA=QWORD |00000037:660F3A600E01 | PCMPESTRM XMM1,[RSI],1 |0000003D:66450F3A61DF01 | PCMPESTRI XMM11,XMM15,1 |00000044:66450F3A61DF01 | PCMPESTRI XMM11,XMM15,1,DATA=DWORD |0000004B:664D0F3A61DF01 | PCMPESTRI XMM11,XMM15,1,DATA=QWORD |00000052:6667440F3A611E01 | PCMPESTRI XMM11,[ESI],1 |0000005A:66440F3A62DF01 | PCMPISTRM XMM11,XMM7,1 |00000061:660F3A620C250000000001 | PCMPISTRM XMM1,[0],1 |0000006C:66410F3A63CF01 | PCMPISTRI XMM1,XMM15,1 |00000073:66460F3A631C0E01 | PCMPISTRI XMM11,[RSI+R9],1 | |ENDPROGRAM t3820`

Expected messages t3820.out
  `I0180 Assembling source file "t3820.htm". I0270 Assembling source "t3820". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3820". "t3820.htm"{70} I0510 Assembling program pass 1. "t3820.htm"{70} I0530 Assembling program pass 2 - final. "t3820.htm"{70} I0660 16bit TINY BIN file "t3820.bin" created, size=315. "t3820.htm"{120} I0650 Program "t3820" assembled in 2 passes with errorlevel 0. "t3820.htm"{120} I0750 Source "t3820" (138 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3820.htm.lst" created, size=3163. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲