| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3104: Machine instructions AND ANDB ANDW ANDD ANDQ in 16bit mode

Tested procedures
  IigAND IigANDB IigANDW IigANDD IigANDQ

Source & expected listing t3104.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=36,CPU=386 | |t3104 PROGRAM FORMAT=BIN,IMAGEBASE=0,LISTMAP=OFF,LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:2402 | AND AL,2 |0002:80E002 | AND AL,2,CODE=LONG |0005:250200 | AND AX,2 |0008:83E002 | AND AX,2,CODE=LONG |000B:6683E002 | AND EAX,2 |000F:662502000000 | AND EAX,2,CODE=SHORT |0015:80E102 | AND CL,2 |0018:8026[8600]02 | AND [MemByte],2 |001D:83E102 | AND CX,2 |0020:81E10200 | AND CX,2,IMM=WORD |0024:8326[8400]02 | AND [MemWord],2 |0029:8126[8400]0200 | AND [MemWord],2,IMM=WORD |002F:6683E102 | AND ECX,2 |0033:6681E102000000 | AND ECX,2,IMM=DWORD |003A:668326[8000]02 | AND [MemDword],2 |0040:668126[8000]02000000 | AND [MemDword],2,IMM=DWORD |0049:802502 | ANDB [DI],2 |004C:832502 | ANDW [DI],2 |004F:66832502 | ANDD [DI],2 |0053:20D1 | AND CL,DL |0055:22CA | AND CL,DL,CODE=LONG |0057:20F5 | AND CH,DH |0059:22EE | AND CH,DH,CODE=LONG |005B:21D1 | AND CX,DX |005D:23CA | AND CX,DX,CODE=LONG |005F:6621D1 | AND ECX,EDX |0062:6623CA | AND ECX,EDX,CODE=LONG |0065:220E[8600] | AND CL,[MemByte] |0069:230E[8400] | AND CX,[MemWord] |006D:66230E[8000] | AND ECX,[MemDword] |0072:2016[8600] | AND [MemByte],DL |0076:2116[8400] | AND [MemWord],DX |007A:662116[8000] | AND [MemDword],EDX |007F:90 | ALIGN QWORD |0080:00000000 |MemDword D D |0084:0000 |MemWord D W |0086:00 |MemByte D B | |ENDPROGRAM t3104`

Expected messages t3104.out
  `I0180 Assembling source file "t3104.htm". I0270 Assembling source "t3104". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3104". "t3104.htm"{61} I0510 Assembling program pass 1. "t3104.htm"{61} I0510 Assembling program pass 2. "t3104.htm"{61} I0510 Assembling program pass 3. "t3104.htm"{61} I0530 Assembling program pass 4 - final. "t3104.htm"{61} I0660 16bit TINY BIN file "t3104.bin" created, size=135. "t3104.htm"{100} I0650 Program "t3104" assembled in 4 passes with errorlevel 0. "t3104.htm"{100} I0750 Source "t3104" (120 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3104.htm.lst" created, size=2289. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲