| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t5450: Machine instructions VPSCATTERDD VPSCATTERDQ VPSCATTERQD VPSCATTERQQ

Tested procedures
  IizVPSCATTERDD IizVPSCATTERDQ IizVPSCATTERQD IizVPSCATTERQQ

Source & expected listing t5450.htm.lst
  `| |EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,EVEX=ON,MVEX=ON | |t5450 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:62F27D0BA1540D10<2 | VPSCATTERQD [XMM1+RBP+40h],XMM2,MASK=K3 |00000008:62F27D2BA1540D10<2 | VPSCATTERQD [YMM1+RBP+40h],XMM2,MASK=K3 |00000010:62F27D4BA1540D10<2 | VPSCATTERQD [ZMM1+RBP+40h],YMM2,MASK=K3 |00000018:62F2FD0BA1540D08<3 | VPSCATTERQQ [XMM1+RBP+40h],XMM2,MASK=K3 |00000020:62F2FD2BA1540D08<3 | VPSCATTERQQ [YMM1+RBP+40h],YMM2,MASK=K3 |00000028:62F2FD4BA1540D08<3 | VPSCATTERQQ [ZMM1+RBP+40h],ZMM2,MASK=K3 |00000030:62F2FD0BA0540D08<3 | VPSCATTERDQ [XMM1+RBP+40h],XMM2,MASK=K3 |00000038:62F2FD2BA0540D08<3 | VPSCATTERDQ [XMM1+RBP+40h],YMM2,MASK=K3 |00000040:62F2FD4BA0540D08<3 | VPSCATTERDQ [YMM1+RBP+40h],ZMM2,MASK=K3 |00000048:62F2F90BA0540D08<3 | VPSCATTERDQ [ZMM1+RBP+40h],ZMM2,MASK=K3 ; MVEX only version. |00000050:62F27D0BA0540D10<2 | VPSCATTERDD [XMM1+RBP+40h],XMM2,MASK=K3 |00000058:62F27D2BA0540D10<2 | VPSCATTERDD [YMM1+RBP+40h],YMM2,MASK=K3 |00000060:62F27D4BA0540D10<2 | VPSCATTERDD [ZMM1+RBP+40h],ZMM2,MASK=K3 |00000068:62F2790BA0540D10<2 | VPSCATTERDD [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=0 ; No conversion. |00000070:62F2794BA0540D40 | VPSCATTERDD [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=4 ; {uint8}. |00000078:62F2795BA0540D40 | VPSCATTERDD [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=5 ; {sint8}. |00000080:62F2796BA0540D20<1 | VPSCATTERDD [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=6 ; {uint16}. |00000088:62F2797BA0540D20<1 | VPSCATTERDD [ZMM1+RBP+40h],ZMM2,MASK=K3,PREFIX=MVEX,OPER=7 ; {sint16}. | |ENDPROGRAM t5450`

Expected messages t5450.out
  `I0180 Assembling source file "t5450.htm". I0270 Assembling source "t5450". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t5450". "t5450.htm"{58} I0510 Assembling program pass 1. "t5450.htm"{58} I0530 Assembling program pass 2 - final. "t5450.htm"{58} I0660 16bit TINY BIN file "t5450.bin" created, size=144. "t5450.htm"{78} I0650 Program "t5450" assembled in 2 passes with errorlevel 0. "t5450.htm"{78} I0750 Source "t5450" (96 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t5450.htm.lst" created, size=1783. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲