| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t3155: Machine instruction JMPE in 16bit mode

Tested procedures
  IisJMPE

Source & expected listing t3155.htm.lst
  `| | EUROASM LIST=ON, DUMP=ON, DUMPWIDTH=38, CPU=X64, UNDOC=ON | |t3155 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode16] |[Mode16] SEGMENT WIDTH=16,PURPOSE=CODE |0000:00000000 |MemDword DD D |0004:0000 |MemWord DW W |0006:0FB80D00 | JMPE $+0x11 |000A:0FB8DAEE | JMPE $-0x1122 |000E:660FB8C6DDEEFF | JMPE $-0x112233 |0015:0FB8(1100) | JMPE 0x11 |0019:0FB8(2211) | JMPE 0x1122 |001D:660FB8(33221100) | JMPE 0x112233 |0024:0F00F2 | JMPE DX |0027:660F00F2 | JMPE EDX |002B:0F0036[0400] | JMPE [MemWord] |0030:660F0036[0000] | JMPE [MemDword] |0036:0F0034 | JMPE [SI] |0039:0F0034 | JMPE [SI],DATA=WORD |003C:660F0034 | JMPE [SI],DATA=DWORD |0040:0F00B40000 | JMPE [SI],DISP=WORD |0045:670F0036 | JMPE [ESI] |0049:670F0036 | JMPE [ESI],DATA=WORD |004D:66670F0036 | JMPE [ESI],DATA=DWORD |0052:670F00B600000000 | JMPE [ESI],DISP=DWORD | |ENDPROGRAM t3155`

Expected messages t3155.out
  `I0180 Assembling source file "t3155.htm". I0270 Assembling source "t3155". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t3155". "t3155.htm"{49} I0510 Assembling program pass 1. "t3155.htm"{49} I0510 Assembling program pass 2. "t3155.htm"{49} I0530 Assembling program pass 3 - final. "t3155.htm"{49} I0660 16bit TINY BIN file "t3155.bin" created, size=90. "t3155.htm"{71} I0650 Program "t3155" assembled in 3 passes with errorlevel 0. "t3155.htm"{71} I0750 Source "t3155" (90 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t3155.htm.lst" created, size=1425. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲