| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t4315: Machine instructions BNDLDX BNDSTX BNDMOV

Tested procedures
  IisBNDLDX IisBNDSTX IisBNDMOV

Source & expected listing t4315.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=34,DUMPALL=OFF,CPU=X64,MPX=ENABLED | |t4315 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode32] |[Mode32] SEGMENT WIDTH=32,PURPOSE=CODE |00000000:0F1A0E | BNDLDX BND1,[ESI] |00000003:0F1A0C16 | BNDLDX BND1,[ESI+EDX] |00000007:0F1B17 | BNDSTX [EDI],BND2 |0000000A:0F1B1417 | BNDSTX [EDI+EDX],BND2 |0000000E:660F1ACA | BNDMOV BND1,BND2 |00000012:660F1BD1 | BNDMOV BND1,BND2,CODE=LONG |00000016:660F1A0E | BNDMOV BND1,[ESI] |0000001A:660F1B17 | BNDMOV [EDI],BND2 |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:0F1A0E | BNDLDX BND1,[RSI] |00000003:0F1A0C16 | BNDLDX BND1,[RSI+RDX] |00000007:430F1A0C2A | BNDLDX BND1,[R10+R13] |0000000C:0F1B17 | BNDSTX [RDI],BND2 |0000000F:0F1B1417 | BNDSTX [RDI+RDX],BND2 |00000013:430F1B1433 | BNDSTX [R11+R14],BND2 |00000018:660F1ACA | BNDMOV BND1,BND2 |0000001C:660F1BD1 | BNDMOV BND1,BND2,CODE=LONG |00000020:660F1A0E | BNDMOV BND1,[RSI] |00000024:660F1B17 | BNDMOV [RDI],BND2 | |ENDPROGRAM t4315`

Expected messages t4315.out
  `I0180 Assembling source file "t4315.htm". I0270 Assembling source "t4315". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t4315". "t4315.htm"{55} I0510 Assembling program pass 1. "t4315.htm"{55} I0530 Assembling program pass 2 - final. "t4315.htm"{55} I0660 16bit TINY BIN file "t4315.bin" created, size=72. "t4315.htm"{76} I0650 Program "t4315" assembled in 2 passes with errorlevel 0. "t4315.htm"{76} I0750 Source "t4315" (94 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t4315.htm.lst" created, size=1407. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲