| Index | Manual | Download | Source | Macros | Embedded word Case ins.
Sitemap | Links | Forum | Tests | Projects

# Test t6240: Machine instructions VPREFETCH0 VPREFETCH1 VPREFETCH2 VPREFETCHE0 VPREFETCHE1 VPREFETCHE2

Tested procedures
  IiyVPREFETCH0 IiyVPREFETCH1 IiyVPREFETCH2 IiyVPREFETCHE0 IiyVPREFETCHE1 IiyVPREFETCHE2

Source & expected listing t6240.htm.lst
  `| | EUROASM LIST=ON,DUMP=ON,DUMPWIDTH=30,CPU=X64,SIMD=AVX512,MVEX=ON | |t6240 PROGRAM FORMAT=BIN, LISTMAP=OFF, LISTGLOBALS=OFF |[Mode64] |[Mode64] SEGMENT WIDTH=64,PURPOSE=CODE |00000000:C5F8184D40 | VPREFETCH0 [RBP+40h] |00000005:C5F8185540 | VPREFETCH1 [RBP+40h] |0000000A:C5F8185D40 | VPREFETCH2 [RBP+40h] |0000000F:C5F8186D40 | VPREFETCHE0 [RBP+40h] |00000014:C5F8187540 | VPREFETCHE1 [RBP+40h] |00000019:C5F8187D40 | VPREFETCHE2 [RBP+40h] |0000001E:C4E178184D40 | VPREFETCH0 [RBP+40h],PREFIX=VEX3 |00000024:C4E178185540 | VPREFETCH1 [RBP+40h],PREFIX=VEX3 |0000002A:C4E178185D40 | VPREFETCH2 [RBP+40h],PREFIX=VEX3 |00000030:C4E178186D40 | VPREFETCHE0 [RBP+40h],PREFIX=VEX3 |00000036:C4E178187540 | VPREFETCHE1 [RBP+40h],PREFIX=VEX3 |0000003C:C4E178187D40 | VPREFETCHE2 [RBP+40h],PREFIX=VEX3 |00000042:62F17808184D01<6 | VPREFETCH0 [RBP+40h],PREFIX=MVEX |00000049:62F17808185501<6 | VPREFETCH1 [RBP+40h],PREFIX=MVEX |00000050:62F17808185D01<6 | VPREFETCH2 [RBP+40h],PREFIX=MVEX |00000057:62F17808186D01<6 | VPREFETCHE0 [RBP+40h],PREFIX=MVEX |0000005E:62F17808187501<6 | VPREFETCHE1 [RBP+40h],PREFIX=MVEX |00000065:62F17808187D01<6 | VPREFETCHE2 [RBP+40h],PREFIX=MVEX | |ENDPROGRAM t6240`

Expected messages t6240.out
  `I0180 Assembling source file "t6240.htm". I0270 Assembling source "t6240". I0310 Assembling source pass 1. I0330 Assembling source pass 2 - final. I0470 Assembling program "t6240". "t6240.htm"{64} I0510 Assembling program pass 1. "t6240.htm"{64} I0530 Assembling program pass 2 - final. "t6240.htm"{64} I0660 16bit TINY BIN file "t6240.bin" created, size=108. "t6240.htm"{84} I0650 Program "t6240" assembled in 2 passes with errorlevel 0. "t6240.htm"{84} I0750 Source "t6240" (102 lines) assembled in 2 passes with errorlevel 0. I0860 Listing file "t6240.htm.lst" created, size=1417. I0990 EuroAssembler terminated with errorlevel 0.`

▲Back to the top▲